
Results text file opened in Study.
File: Fda_Results.txt opened on Sat Apr 27 09:35:50 2024
	(C:\Users\q0hecrjn.HQ-FOA\Richard\HEC-FDA\2.0\TroubleshootingCompute\Bear Creek Mix EAD Comparison\BearCreek_Mix\Fda_Results.txt)
------------------------------------------------------------------------------------------------------------------------
Report Expected Annual Damage by Plans and Analysis Years.
Study:	BearCreek_Mix
Monetary Units:	$1,000's
Version 1.4.3, January 1, 2021;  Less Simple Method  (0.010)                                                                                                                        
Plan	Plan Description	2021	
 Without	Without project condition	    439.31	
 01FW	Floodwall	    194.78	
 02FW+GEO	Floodwall and geotech	    235.86	
 03FW+IE	Floodwall and Interior / Exterior	     88.73	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	    128.62	
 05TransQ_G	Transform flow, Base yr graphical	    546.26	
 06TransQ_A	Transform flow, Base yr analytical	    523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	    235.86	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	    128.62	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	    131.06	
 10WspStage	Without plan but with stage profiles	    623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	    215.16	
 12As	Analytical using synthetic ordinates	    553.88	
 13Am	Log Pearson III Analytic from Moments	    547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	    600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	    622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	    588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	    594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	    196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	    237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	    564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	      4.38	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	    235.89	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	    595.89	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	    621.35	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	    621.33	



Report Expected Annual Damage by Plans and Categories.
Study:	BearCreek_Mix
Year:	2021
Monetary Units:	$1,000's
Version 1.4.3, January 1, 2021;  Less Simple Method  (0.010)                                                                                                                        
Plan	Plan Description	APT	AUTO	COMM	PUB	RES	Total
 Without	Without project condition	      285.64	       11.96	       95.84	        0.24	       45.63	      439.31	
 01FW	Floodwall	       73.67	        8.53	       90.22	        0.23	       22.13	      194.78	
 02FW+GEO	Floodwall and geotech	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 03FW+IE	Floodwall and Interior / Exterior	       52.92	        4.38	       17.69	        0.00	       13.74	       88.73	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 05TransQ_G	Transform flow, Base yr graphical	      406.78	        9.98	       71.10	        0.23	       58.17	      546.26	
 06TransQ_A	Transform flow, Base yr analytical	      386.34	       10.60	       67.64	        0.20	       58.49	      523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	       83.94	        6.03	       19.96	        0.00	       21.12	      131.06	
 10WspStage	Without plan but with stage profiles	      447.81	       12.81	       94.39	        0.55	       68.21	      623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	       82.09	        9.45	       98.78	        0.26	       24.59	      215.16	
 12As	Analytical using synthetic ordinates	      382.70	       13.33	       95.50	        0.21	       62.14	      553.88	
 13Am	Log Pearson III Analytic from Moments	      378.79	       13.14	       94.18	        0.20	       61.25	      547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	      425.11	       12.79	       97.76	        0.22	       64.38	      600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	      446.95	       12.87	       94.52	        0.52	       68.05	      622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	      422.10	       12.36	       90.05	        0.19	       63.41	      588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	      434.26	       12.03	       82.78	        0.48	       64.91	      594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	       74.03	        8.68	       91.33	        0.20	       22.28	      196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	      103.80	       10.28	       93.60	        0.20	       29.37	      237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	      420.37	       11.38	       71.00	        0.12	       61.54	      564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	        4.36	        0.00	        0.00	        0.00	        0.03	        4.38	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	      103.02	       10.16	       93.28	        0.23	       29.19	      235.89	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	      423.94	       12.68	       94.84	        0.24	       64.19	      595.89	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	      435.00	       13.79	      104.68	        0.28	       67.60	      621.35	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	      434.99	       13.79	      104.67	        0.28	       67.60	      621.33	


Report Expected Annual Damage by Plans and Categories.
Study:	BearCreek_Mix
Year:	2021
Monetary Units:	$1,000's
Version 1.4.3, January 1, 2021;  Less Simple Method  (0.010)                                                                                                                        
Plan	Plan Description	APT	AUTO	COMM	PUB	RES	Total
 Without	Without project condition	      245.58	       11.92	       95.48	        0.24	       45.46	      398.68	
 01FW	Floodwall	       73.67	        8.53	       90.22	        0.23	       22.13	      194.78	
 02FW+GEO	Floodwall and geotech	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 03FW+IE	Floodwall and Interior / Exterior	       52.92	        4.38	       17.69	        0.00	       13.74	       88.73	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 05TransQ_G	Transform flow, Base yr graphical	      406.78	        9.98	       71.10	        0.23	       58.17	      546.26	
 06TransQ_A	Transform flow, Base yr analytical	      386.34	       10.60	       67.64	        0.20	       58.49	      523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	       83.94	        6.03	       19.96	        0.00	       21.12	      131.06	
 10WspStage	Without plan but with stage profiles	      447.81	       12.81	       94.39	        0.55	       68.21	      623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	       82.09	        9.45	       98.78	        0.26	       24.59	      215.16	
 12As	Analytical using synthetic ordinates	      382.70	       13.33	       95.50	        0.21	       62.14	      553.88	
 13Am	Log Pearson III Analytic from Moments	      378.79	       13.14	       94.18	        0.20	       61.25	      547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	      425.11	       12.79	       97.76	        0.22	       64.38	      600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	      446.95	       12.87	       94.52	        0.52	       68.05	      622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	      422.10	       12.36	       90.05	        0.19	       63.41	      588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	      434.26	       12.03	       82.78	        0.48	       64.91	      594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	       74.03	        8.68	       91.33	        0.20	       22.28	      196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	      103.80	       10.28	       93.60	        0.20	       29.37	      237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	      420.37	       11.38	       71.00	        0.12	       61.54	      564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	        4.36	        0.00	        0.00	        0.00	        0.03	        4.38	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	      103.02	       10.16	       93.28	        0.23	       29.19	      235.89	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	      423.94	       12.68	       94.84	        0.24	       64.19	      595.89	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	      435.00	       13.79	      104.68	        0.28	       67.60	      621.35	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	      434.99	       13.79	      104.67	        0.28	       67.60	      621.33	


Report Expected Annual Damage by Plans and Categories.
Study:	BearCreek_Mix
Year:	2021
Monetary Units:	$1,000's
Version 1.4.3, January 1, 2021;  Less Simple Method  (0.010)                                                                                                                        
Plan	Plan Description	APT	AUTO	COMM	PUB	RES	Total
 Without	Without project condition	      262.42	       11.93	       95.61	        0.24	       45.52	      415.73	
 01FW	Floodwall	       73.67	        8.53	       90.22	        0.23	       22.13	      194.78	
 02FW+GEO	Floodwall and geotech	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 03FW+IE	Floodwall and Interior / Exterior	       52.92	        4.38	       17.69	        0.00	       13.74	       88.73	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 05TransQ_G	Transform flow, Base yr graphical	      406.78	        9.98	       71.10	        0.23	       58.17	      546.26	
 06TransQ_A	Transform flow, Base yr analytical	      386.34	       10.60	       67.64	        0.20	       58.49	      523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	      103.00	       10.16	       93.28	        0.23	       29.19	      235.86	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	       81.75	        5.97	       20.25	        0.00	       20.65	      128.62	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	       83.94	        6.03	       19.96	        0.00	       21.12	      131.06	
 10WspStage	Without plan but with stage profiles	      447.81	       12.81	       94.39	        0.55	       68.21	      623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	       82.09	        9.45	       98.78	        0.26	       24.59	      215.16	
 12As	Analytical using synthetic ordinates	      382.70	       13.33	       95.50	        0.21	       62.14	      553.88	
 13Am	Log Pearson III Analytic from Moments	      378.79	       13.14	       94.18	        0.20	       61.25	      547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	      425.11	       12.79	       97.76	        0.22	       64.38	      600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	      446.95	       12.87	       94.52	        0.52	       68.05	      622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	      422.10	       12.36	       90.05	        0.19	       63.41	      588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	      434.26	       12.03	       82.78	        0.48	       64.91	      594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	       74.03	        8.68	       91.33	        0.20	       22.28	      196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	      103.80	       10.28	       93.60	        0.20	       29.37	      237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	      420.37	       11.38	       71.00	        0.12	       61.54	      564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	        4.36	        0.00	        0.00	        0.00	        0.03	        4.38	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	      103.02	       10.16	       93.28	        0.23	       29.19	      235.89	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	      423.94	       12.68	       94.84	        0.24	       64.19	      595.89	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	      435.00	       13.79	      104.68	        0.28	       67.60	      621.35	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	      434.99	       13.79	      104.67	        0.28	       67.60	      621.33	


Report Expected Annual Damage by Plans and Analysis Years.
Study:	BearCreek_Mix
Monetary Units:	$1,000's
Version 1.4.3, January 1, 2021;  Less Simple Method  (0.010)                                                                                                                        
Plan	Plan Description	2021	
 Without	Without project condition	    415.73	
 01FW	Floodwall	    197.61	
 02FW+GEO	Floodwall and geotech	    237.94	
 03FW+IE	Floodwall and Interior / Exterior	     90.83	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	    129.54	
 05TransQ_G	Transform flow, Base yr graphical	    546.26	
 06TransQ_A	Transform flow, Base yr analytical	    523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	    237.94	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	    129.54	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	    131.06	
 10WspStage	Without plan but with stage profiles	    623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	    218.68	
 12As	Analytical using synthetic ordinates	    553.88	
 13Am	Log Pearson III Analytic from Moments	    547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	    600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	    622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	    588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	    594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	    196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	    237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	    564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	      4.51	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	    237.97	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	    439.31	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	    460.59	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	    460.57	



