NOTE 15301:  Began computing simulation run "Jan_2010" at time 29Aug2025, 10:07:53.
NOTE 20364:  Found no parameter problems in meteorologic model "LAPW_Interp_PRISM_Bias".
WARNING 45220:  No plant uptake method selected for subbasin "ArroyoSeco_S10".  There will be no transpiration for loss method: Deficit and Constant.
WARNING 40334:  No canopy method selected for use with Deficit Constant loss method in subbasin "ArroyoSeco_S10".  No transpiration calculations will be performed.
NOTE 40049:  Found no parameter problems in basin model "Jan_2010".
WARNING 40017:  Observed Discharge gage "ArroyoSeco_Gage" at element "Outlet" has some missing data.
NOTE 45913:  Clark Tc=1.60 hr, R=0.75 hr for period ending at 18Jan2010, 13:00 for subbasin "ArroyoSeco_S10".
NOTE 45913:  Clark Tc=1.60 hr, R=0.75 hr for period ending at 18Jan2010, 21:00 for subbasin "ArroyoSeco_S10".
NOTE 45913:  Clark Tc=1.60 hr, R=0.75 hr for period ending at 18Jan2010, 22:00 for subbasin "ArroyoSeco_S10".
NOTE 45913:  Clark Tc=1.60 hr, R=0.75 hr for period ending at 18Jan2010, 23:00 for subbasin "ArroyoSeco_S10".
NOTE 45913:  Clark Tc=1.60 hr, R=0.75 hr for period ending at 19Jan2010, 00:00 for subbasin "ArroyoSeco_S10".
NOTE 15302:  Finished computing simulation run "Jan_2010" at time 29Aug2025, 10:07:56.
NOTE 15312:  The total runtime for this simulation is 00:03.
