Basin: 01_Pre_2006_01_WFS
     Description: with wetting front suction
     Last Modified Date: 16 October 2024
     Last Modified Time: 17:04:21
     Version: 4.13
     Filepath Separator: \
     Unit System: English
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: No
End:

Subbasin: AS100_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.27195737611951
     Longitude Degrees: -118.11527777777778
     Canvas X: -6570116.796722206
     Canvas Y: 4853807.962061676
     Area: 0.725799
     Downstream: AS250_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.78
     Hydraulic Conductivity: 0.37

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.76
     Storage Coefficient: 0.76
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS150_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.261828585330505
     Longitude Degrees: -118.10902551316501
     Canvas X: -6569135.862734917
     Canvas Y: 4849757.577727089
     Area: 0.5105101
     Downstream: AS250_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.73
     Hydraulic Conductivity: 0.34

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.53
     Storage Coefficient: 0.53
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS200_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.2532464362599
     Longitude Degrees: -118.1129932559969
     Canvas X: -6571019.270030293
     Canvas Y: 4846968.967800611
     Area: 0.453400
     Downstream: AS250_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 4.3
     Hydraulic Conductivity: 0.22

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.71
     Storage Coefficient: 0.71
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS250_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6578880.9311937
     Canvas Y: 4853691.85840107
     From Canvas X: -6571839.362044833
     From Canvas Y: 4850282.256497408
     Downstream: AS350_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 9282.15
     Energy Slope: 0.062
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS250_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS300_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.276374416907096
     Longitude Degrees: -118.1317690944625
     Canvas X: -6574539.71997648
     Canvas Y: 4856521.637782386
     Area: 1.467999
     Downstream: AS350_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.56
     Hydraulic Conductivity: 0.39

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.73
     Storage Coefficient: 0.73
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS250_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.263867107044994
     Longitude Degrees: -118.12985540376727
     Canvas X: -6575040.173993306
     Canvas Y: 4851925.609163866
     Area: 0.854402
     Downstream: AS350_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.76
     Hydraulic Conductivity: 0.34

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.69
     Storage Coefficient: 0.69
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS350_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6581771.680633762
     Canvas Y: 4849170.429789692
     From Canvas X: -6578880.9311937
     From Canvas Y: 4853691.85840107
     Downstream: AS425_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 10904.86
     Energy Slope: 0.060
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS350_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS400_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.25544115194837
     Longitude Degrees: -118.1343539457704
     Canvas X: -6577065.80228421
     Canvas Y: 4849229.873952462
     Area: 0.965599
     Downstream: AS425_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.67
     Hydraulic Conductivity: 0.36

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.75
     Storage Coefficient: 0.75
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS350_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.26286210197915
     Longitude Degrees: -118.15115567548442
     Canvas X: -6581338.90775579
     Canvas Y: 4853041.355598779
     Area: 0.813401
     Downstream: AS425_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.49
     Hydraulic Conductivity: 0.39

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.78
     Storage Coefficient: 0.78
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS425_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6581956.985085048
     Canvas Y: 4848688.638216348
     From Canvas X: -6581771.680633762
     From Canvas Y: 4849170.429789692
     Downstream: AS420_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 559.06
     Energy Slope: 0.052
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS425_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS450_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.24280835057992
     Longitude Degrees: -118.12344334607924
     Canvas X: -6574951.507747008
     Canvas Y: 4843966.568658819
     Area: 2.639699
     Downstream: AS420_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.83
     Hydraulic Conductivity: 0.46

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.26
     Storage Coefficient: 1.26
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS420_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6582920.568231735
     Canvas Y: 4848132.724862491
     From Canvas X: -6581956.985085048
     From Canvas Y: 4848688.638216348
     Downstream: AS550_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 1268.04
     Energy Slope: 0.044
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS420_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS500_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.2416216894413
     Longitude Degrees: -118.14790317788487
     Canvas X: -6582189.322974719
     Canvas Y: 4845236.295608752
     Area: 0.430500
     Downstream: AS550_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 4.35
     Hydraulic Conductivity: 0.2

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.50
     Storage Coefficient: 0.50
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS420_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.250012091800436
     Longitude Degrees: -118.15057218471135
     Canvas X: -6582257.313884755
     Canvas Y: 4848415.314150704
     Area: 0.048479
     Downstream: AS550_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 4.66
     Hydraulic Conductivity: 0.06

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.30
     Storage Coefficient: 0.30
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS550_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6589739.77203906
     Canvas Y: 4850875.230741523
     From Canvas X: -6582920.568231735
     From Canvas Y: 4848132.724862491
     Downstream: AS700_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 16168.96
     Energy Slope: 0.036
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS550_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS640_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.26317525382644
     Longitude Degrees: -118.17030181408518
     Canvas X: -6586897.343777988
     Canvas Y: 4854479.592910877
     Area: 0.593999
     Downstream: AS685_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.8
     Hydraulic Conductivity: 0.38

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.62
     Storage Coefficient: 0.62
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS660_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.257300687403635
     Longitude Degrees: -118.16408958090759
     Canvas X: -6585583.229506599
     Canvas Y: 4851952.745829511
     Area: 0.504701
     Downstream: AS685_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 5.83
     Hydraulic Conductivity: 0.06

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.84
     Storage Coefficient: 0.84
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS685_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6589146.797794945
     Canvas Y: 4850949.352522038
     From Canvas X: -6588590.884441086
     From Canvas Y: 4851097.596083066
     Downstream: AS680_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 669.95
     Energy Slope: 0.098
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS685_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS600_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.262072050263
     Longitude Degrees: -118.17966836430404
     Canvas X: -6589723.069010047
     Canvas Y: 4854735.275860767
     Area: 0.491601
     Downstream: AS680_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.28
     Hydraulic Conductivity: 0.59

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.60
     Storage Coefficient: 0.60
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS680_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6589739.77203906
     Canvas Y: 4850875.230741523
     From Canvas X: -6589146.797794945
     From Canvas Y: 4850949.352522038
     Downstream: AS700_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 685.04
     Energy Slope: 0.121
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS680_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS550_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.247738440985934
     Longitude Degrees: -118.16329684394798
     Canvas X: -6586162.510276124
     Canvas Y: 4848485.5690250425
     Area: 0.957398
     Downstream: AS700_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 5.35
     Hydraulic Conductivity: 0.11

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.15
     Storage Coefficient: 1.15
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS680_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.25206047980445
     Longitude Degrees: -118.17453674944323
     Canvas X: -6589075.260292041
     Canvas Y: 4850806.982319212
     Area: 0.0310880
     Downstream: AS700_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.03
     Capillarity Method: SUCTION
     Wetting Front Suction: 7.32
     Hydraulic Conductivity: 0.3

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.16
     Storage Coefficient: 0.16
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS700_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6590443.928953947
     Canvas Y: 4850059.891155865
     From Canvas X: -6589739.77203906
     From Canvas Y: 4850875.230741523
     Downstream: AS740_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 2563.98
     Energy Slope: 0.030
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS700_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS720_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.25931339218979
     Longitude Degrees: -118.18746766417289
     Canvas X: -6592232.131559749
     Canvas Y: 4854291.818189334
     Area: 0.623099
     Downstream: AS740_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.3
     Hydraulic Conductivity: 0.59

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.68
     Storage Coefficient: 0.68
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS700_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.25243712472987
     Longitude Degrees: -118.17866474775923
     Canvas X: -6590247.582151748
     Canvas Y: 4851227.619765088
     Area: 0.079402
     Downstream: AS740_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 5.09
     Hydraulic Conductivity: 0.46

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.24
     Storage Coefficient: 0.24
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS740_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6592445.217027835
     Canvas Y: 4848985.125338406
     From Canvas X: -6590443.928953947
     From Canvas Y: 4850059.891155865
     Downstream: AS800_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 4112.86
     Energy Slope: 0.021
     Mannings n: 0.040
     Left Mannings n: 0.050
     Right Mannings n: 0.050
     Cross Section Name: AS740_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS760_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.252450306929795
     Longitude Degrees: -118.19753559812129
     Canvas X: -6595751.511272322
     Canvas Y: 4852541.502883083
     Area: 1.227701
     Downstream: AS800_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.98
     Hydraulic Conductivity: 0.14

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.04
     Storage Coefficient: 1.04
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS740_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.24709772511396
     Longitude Degrees: -118.18071408584414
     Canvas X: -6591298.371863692
     Canvas Y: 4849464.490747922
     Area: 0.147499
     Downstream: AS800_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 4.83
     Hydraulic Conductivity: 0.16

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.47
     Storage Coefficient: 0.47
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS800_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6591481.633881148
     Canvas Y: 4845130.792751658
     From Canvas X: -6592445.217027835
     From Canvas Y: 4848985.125338406
     Downstream: AS900_R

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 6234.91
     Energy Slope: 0.028
     Mannings n: 0.040
     Left Mannings n: 0.050
     Right Mannings n: 0.050
     Cross Section Name: AS800_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS800_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.24024012688277
     Longitude Degrees: -118.18789716650619
     Canvas X: -6593975.909134888
     Canvas Y: 4847515.84777101
     Area: 0.883000
     Downstream: AS900_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.03
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.78
     Hydraulic Conductivity: 0.4

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.85
     Storage Coefficient: 0.85
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Subbasin: AS850_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.238129043868554
     Longitude Degrees: -118.1678839864334
     Canvas X: -6588315.5306693325
     Canvas Y: 4845374.518282446
     Area: 0.635899
     Downstream: AS900_R

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 4.73
     Hydraulic Conductivity: 0.04

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.95
     Storage Coefficient: 0.95
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Reach: AS900_R
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6592593.460588864
     Canvas Y: 4840349.937908479
     From Canvas X: -6591481.633881148
     From Canvas Y: 4845130.792751658
     Downstream: ArroyoSeco_USGS

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 9136.15
     Energy Slope: 0.026
     Mannings n: 0.050
     Left Mannings n: 0.060
     Right Mannings n: 0.060
     Cross Section Name: AS900_R
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 4.92
     Number Subreaches: 1
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: AS900_Sub
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:53:23
     Latitude Degrees:  34.22927161535514
     Longitude Degrees: -118.18126950437417
     Canvas X: -6592972.612803216
     Canvas Y: 4843142.245818971
     Area: 0.976900
     Downstream: ArroyoSeco_USGS

     Discretization: Structured
     File: 01_Pre_2006_01_WFS.sqlite
     Projection: 5070
     Cell Size: 2000.0

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Green and Ampt
     Percent Impervious Area: 0
     Initial Variable: Initial Deficit
     Moisture Deficit: 0.04
     Capillarity Method: SUCTION
     Wetting Front Suction: 3.95
     Hydraulic Conductivity: 0.32

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.03
     Storage Coefficient: 1.03
     Time Area Method: Default

     Baseflow: Recession
     Recession Factor: 0.15
     Initial Flow/Area Ratio: 0.00
     Threshold Flow to Peak Ratio: 0.15
End:

Sink: ArroyoSeco_USGS
     Description: Arroyo Seco NR Pasadena CA - 11098000
     Last Modified Date: 16 October 2024
     Last Modified Time: 16:52:04
     Canvas X: -6592593.460588864
     Canvas Y: 4840349.937908479
     Observed Hydrograph Gage: ArroyoSeco_USGS
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     Element Layer:
          Name: Reaches
          Layer shown: Yes
     End Layer:
     2D Connection Layer:
          Layer shown: No
     End Layer:
     Element Layer:
          Name: Subbasins
          Layer shown: Yes
     End Layer:
     Discretization Layer:
          Layer shown: No
     End Layer:
     Breakpoint Layer:
          Layer shown: No
     End Layer:
     Base Layer:
          Name: Identified Streams
          Layer shown: Yes
          Properties Filename: maps\streams4000152562024.xml
     End Layer:
     Base Layer:
          Name: Flow Accumulation
          Layer shown: Yes
          Properties Filename: maps\flowaccum4000152562024.xml
     End Layer:
     Base Layer:
          Name: Flow Direction
          Layer shown: Yes
          Properties Filename: maps\flowdir4000152562024.xml
     End Layer:
     Base Layer:
          Name: Sink Locations
          Layer shown: Yes
          Properties Filename: maps\sinklocs4100152562024.xml
     End Layer:
     Base Layer:
          Name: Sink Fill
          Layer shown: Yes
          Properties Filename: maps\sinkfill4100152562024.xml
     End Layer:
     Base Layer:
          Name: Reconditioned Terrain
          Layer shown: Yes
          Properties Filename: maps\reconditioned4100152562024.xml
     End Layer:
     Base Layer:
          Name: Terrain
          Layer shown: No
          Properties Filename: maps\elevation4100152562024.xml
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["NAD83",DATUM["North_American_Datum_1983",SPHEROID["GRS 1980",6378137,298.257222101004,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","6269"]],PRIMEM["Greenwich",0],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4269"]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["latitude_of_center",23],PARAMETER["longitude_of_center",-96],PARAMETER["standard_parallel_1",29.5],PARAMETER["standard_parallel_2",45.5],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["US survey foot",0.304800609601219,AUTHORITY["EPSG","9003"]],AXIS["Easting",EAST],AXIS["Northing",NORTH]]
     Terrain: USGS_3DEP
     Threshold: 0.402
     Break Point: Arroyo_Seco_USGS
          Description: USGS 11098000
          X Coordinate: -6592806.293334655
          Y Coordinate: 4840136.860177626
     End Break Point:
End:

Basin Schematic Properties:
     Last View N: 4866599.4468137
     Last View S: 4832418.884633065
     Last View W: -6609437.007233566
     Last View E: -6560464.8567408435
     Maximum View N: 4856521.637782386
     Maximum View S: 4840349.937908479
     Maximum View W: -6595751.511272322
     Maximum View E: -6569135.862734917
     Extent Method: Elements
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
