WARNING 41074:  Length for reach "AS425_R" is very short and may cause numeric instabilities.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 622 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1097 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 100 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 173 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1279 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41083:  Celerity in reach "AS250_R" ranged from 0.6 to 2.1 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS250_R" would have increased spatial steps from 3 to 11.
WARNING 41083:  Celerity in reach "AS350_R" ranged from 0.8 to 4.5 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 2 cfs at reach "AS350_R" would have increased spatial steps from 3 to 6.
WARNING 41083:  Celerity in reach "AS425_R" ranged from 1.1 to 4.4 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 3 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS420_R" ranged from 1.1 to 4.8 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS550_R" ranged from 1.0 to 4.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS550_R" would have increased spatial steps from 4 to 9.
WARNING 41083:  Celerity in reach "AS685_R" ranged from 1.0 to 4.3 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS700_R" ranged from 0.7 to 2.9 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41083:  Celerity in reach "AS740_R" ranged from 0.8 to 3.2 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS740_R" would have increased spatial steps from 1 to 3.
WARNING 41083:  Celerity in reach "AS800_R" ranged from 0.8 to 2.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS800_R" would have increased spatial steps from 2 to 6.
WARNING 41083:  Celerity in reach "AS900_R" ranged from 1.0 to 4.0 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS900_R" would have increased spatial steps from 3 to 6.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41083:  Celerity in reach "AS250_R" ranged from 0.7 to 3.8 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 16 cfs at reach "AS250_R" would have increased spatial steps from 3 to 6.
WARNING 41084:  Applying the diffusivity criteria using index flow 174 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 258 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS685_R" ranged from 1.0 to 2.3 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 0 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 26 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 327 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41083:  Celerity in reach "AS250_R" ranged from 0.6 to 2.1 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS250_R" would have increased spatial steps from 3 to 11.
WARNING 41083:  Celerity in reach "AS350_R" ranged from 0.8 to 4.5 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 2 cfs at reach "AS350_R" would have increased spatial steps from 3 to 6.
WARNING 41083:  Celerity in reach "AS425_R" ranged from 1.1 to 4.4 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 3 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS420_R" ranged from 1.1 to 4.8 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS550_R" ranged from 1.0 to 4.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS550_R" would have increased spatial steps from 4 to 9.
WARNING 41083:  Celerity in reach "AS685_R" ranged from 1.0 to 4.3 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS700_R" ranged from 0.7 to 2.9 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41083:  Celerity in reach "AS740_R" ranged from 0.8 to 3.2 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS740_R" would have increased spatial steps from 1 to 3.
WARNING 41083:  Celerity in reach "AS800_R" ranged from 0.8 to 2.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS800_R" would have increased spatial steps from 2 to 6.
WARNING 41083:  Celerity in reach "AS900_R" ranged from 1.0 to 4.0 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS900_R" would have increased spatial steps from 3 to 6.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 668 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1055 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 27 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 107 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1345 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 87 cfs at reach "AS250_R" would have increased spatial steps from 3 to 4.
WARNING 41084:  Applying the diffusivity criteria using index flow 216 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 385 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 41 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 66 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 433 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 114 cfs at reach "AS250_R" would have increased spatial steps from 3 to 4.
WARNING 41084:  Applying the diffusivity criteria using index flow 553 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 871 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 17 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 85 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1099 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41083:  Celerity in reach "AS250_R" ranged from 0.6 to 2.1 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS250_R" would have increased spatial steps from 3 to 11.
WARNING 41083:  Celerity in reach "AS350_R" ranged from 0.8 to 4.5 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 2 cfs at reach "AS350_R" would have increased spatial steps from 3 to 6.
WARNING 41083:  Celerity in reach "AS425_R" ranged from 1.1 to 4.4 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 3 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS420_R" ranged from 1.1 to 4.8 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS550_R" ranged from 1.0 to 4.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS550_R" would have increased spatial steps from 4 to 9.
WARNING 41083:  Celerity in reach "AS685_R" ranged from 1.0 to 4.3 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS700_R" ranged from 0.7 to 2.9 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41083:  Celerity in reach "AS740_R" ranged from 0.8 to 3.2 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS740_R" would have increased spatial steps from 1 to 3.
WARNING 41083:  Celerity in reach "AS800_R" ranged from 0.8 to 2.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS800_R" would have increased spatial steps from 2 to 6.
WARNING 41083:  Celerity in reach "AS900_R" ranged from 1.0 to 4.0 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS900_R" would have increased spatial steps from 3 to 6.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 2382 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 3816 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 520 time steps at reach "AS685_R"; maximum convergence error of 0.082 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 263 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 500 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 5296 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 382 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 677 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 418 time steps at reach "AS685_R"; maximum convergence error of 0.082 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 66 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 111 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 757 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 1711 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 2732 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 520 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 143 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 331 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 3705 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41083:  Celerity in reach "AS250_R" ranged from 0.6 to 2.1 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS250_R" would have increased spatial steps from 3 to 11.
WARNING 41083:  Celerity in reach "AS350_R" ranged from 0.8 to 4.5 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 2 cfs at reach "AS350_R" would have increased spatial steps from 3 to 6.
WARNING 41083:  Celerity in reach "AS425_R" ranged from 1.1 to 4.4 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 3 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS420_R" ranged from 1.1 to 4.8 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS550_R" ranged from 1.0 to 4.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 5 cfs at reach "AS550_R" would have increased spatial steps from 4 to 9.
WARNING 41071:  Flow depth convergence failed 1329 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41083:  Celerity in reach "AS685_R" ranged from 1.0 to 4.3 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41083:  Celerity in reach "AS700_R" ranged from 0.7 to 2.9 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41083:  Celerity in reach "AS740_R" ranged from 0.8 to 3.2 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS740_R" would have increased spatial steps from 1 to 3.
WARNING 41083:  Celerity in reach "AS800_R" ranged from 0.8 to 2.6 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS800_R" would have increased spatial steps from 2 to 6.
WARNING 41083:  Celerity in reach "AS900_R" ranged from 1.0 to 4.0 ft/s.  Specified index celerity was 5 ft/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 6 cfs at reach "AS900_R" would have increased spatial steps from 3 to 6.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41071:  Flow depth convergence failed 492 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 2972 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 112115 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 491 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 869 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 432 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 82 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 140 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 984 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41071:  Flow depth convergence failed 24 time steps at reach "AS350_R"; maximum convergence error of 0.2289 FT.
WARNING 41071:  Flow depth convergence failed 499 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 21627 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 106187 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 61 cfs at reach "AS250_R" would have increased spatial steps from 3 to 4.
WARNING 41084:  Applying the diffusivity criteria using index flow 149 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 266 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 287 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 30 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 47 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 298 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 123 cfs at reach "AS250_R" would have increased spatial steps from 3 to 4.
WARNING 41084:  Applying the diffusivity criteria using index flow 311 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 552 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 406 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 56 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 93 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 620 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41071:  Flow depth convergence failed 12 time steps at reach "AS350_R"; maximum convergence error of 0.2289 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 32741 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 32460 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 442 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 144 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 10000 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 36208 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 420 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 743 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 419 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 71 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 121 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 835 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 711 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1252 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 446 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 114 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 197 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1465 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41071:  Flow depth convergence failed 11 time steps at reach "AS350_R"; maximum convergence error of 0.2289 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 33120 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 33399 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 448 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 140 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 34797 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 53853 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 575 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1015 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 435 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 93 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 161 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1179 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 494 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 874 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 432 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 82 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 140 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 990 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 655 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1154 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 105 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 182 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1347 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 702 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1236 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 445 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 112 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 195 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1447 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 606 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1069 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 98 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 169 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1248 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 670 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1181 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 440 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 107 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 186 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1381 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 622 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1098 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 100 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 173 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1280 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 655 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1154 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 105 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 182 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1347 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 687 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1210 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 442 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 110 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 190 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1417 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 639 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1126 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 102 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 178 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1315 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 638 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1125 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 102 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 177 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1314 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 622 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1097 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 100 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 173 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1280 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 647 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1140 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 104 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 180 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1331 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 630 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1111 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 101 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 175 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1297 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 643 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1133 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 179 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1323 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 643 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1133 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 179 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1324 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 647 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1140 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 104 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 180 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1331 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 641 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1129 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 178 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1319 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 645 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1136 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 179 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1328 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 642 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1131 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 178 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1321 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
WARNING 40017:  Observed Discharge gage "ArroyoSeco_USGS" at element "ArroyoSeco_USGS" has some missing data.
WARNING 41084:  Applying the diffusivity criteria using index flow 642 cfs at reach "AS425_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1131 cfs at reach "AS420_R" would have increased spatial steps from 1 to 2.
WARNING 41071:  Flow depth convergence failed 439 time steps at reach "AS685_R"; maximum convergence error of 0.0905 FT.
WARNING 41084:  Applying the diffusivity criteria using index flow 103 cfs at reach "AS685_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 178 cfs at reach "AS680_R" would have increased spatial steps from 1 to 2.
WARNING 41084:  Applying the diffusivity criteria using index flow 1321 cfs at reach "AS740_R" would have increased spatial steps from 1 to 2.
