Basin: Punxsutawney
     Description: Headwaters to the City of Punxsutawney - Existing Conditions
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:27:10
     Version: 4.14
     Filepath Separator: \
     Unit System: English
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: No
End:

Subbasin: EB Mahoning Creek
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:34:39
     Canvas X: 4261.767876392383
     Canvas Y: -749.4481802782193
     From Canvas X: 3768.5950413223145
     From Canvas Y: -537.1900826446272
     Area: 41
     Downstream: Junction-1

     Discretization: None
     File: Punxsutawney.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Initial+Constant
     Percent Impervious Area: 0.0
     Initial Loss: 1
     Constant Loss Rate: 0.1

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 7
     Storage Coefficient: 11
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.5
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 70
     GW-1 Initial Flow/Area Ratio: 1
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.5
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 100
     GW-2 Initial Flow/Area Ratio: 1
End:

Subbasin: Stump Creek
     Last Modified Date: 2 July 2026
     Last Modified Time: 16:58:07
     Canvas X: 584.2145047274158
     Canvas Y: 1983.4710743801656
     From Canvas X: 566.1157024793389
     From Canvas Y: 1983.4710743801656
     Area: 29
     Downstream: Junction-1

     Discretization: None
     File: Punxsutawney.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Initial+Constant
     Percent Impervious Area: 0.0
     Initial Loss: 1
     Constant Loss Rate: 0.1

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 9
     Storage Coefficient: 12
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.5
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 70
     GW-1 Initial Flow/Area Ratio: 1
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.5
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 100
     GW-2 Initial Flow/Area Ratio: 1
End:

Junction: Junction-1
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:28:35
     Canvas X: 1392.561983471075
     Canvas Y: 330.57851239669435
     From Canvas X: 1392.561983471075
     From Canvas Y: 330.57851239669435
     Downstream: Reach-1
End:

Subbasin: Mahoning Creek Local
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:34:39
     Canvas X: -2719.008264462809
     Canvas Y: 185.95041322314137
     From Canvas X: -2388.4297520661153
     From Canvas Y: -743.8016528925618
     Area: 88
     Downstream: Junction-2

     Discretization: None
     File: Punxsutawney.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Initial+Constant
     Percent Impervious Area: 0.0
     Initial Loss: 1
     Constant Loss Rate: 0.1

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 10
     Storage Coefficient: 13
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.5
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 70
     GW-1 Initial Flow/Area Ratio: 1
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.5
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 100
     GW-2 Initial Flow/Area Ratio: 1
End:

Reach: Reach-1
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:37:37
     Canvas X: -1210.7438016528922
     Canvas Y: -2809.9173553718992
     From Canvas X: 1392.561983471075
     From Canvas Y: 330.57851239669435
     Downstream: Junction-2

     Route: Lag
     Initial Variable: Combined Inflow
     Lag: 300
     Channel Loss: None
End:

Junction: Junction-2
     Last Modified Date: 27 January 2025
     Last Modified Time: 15:28:35
     Canvas X: -1210.7438016528922
     Canvas Y: -2809.9173553718992
     From Canvas X: -1210.7438016528922
     From Canvas Y: -2809.9173553718992
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
End:

Basin Spatial Properties:
End:

Basin Schematic Properties:
     Last View N: 1983.4710743801656
     Last View S: -2809.9173553718992
     Last View W: -2719.008264462809
     Last View E: 4261.767876392383
     Maximum View N: 1983.4710743801656
     Maximum View S: -2809.9173553718992
     Maximum View W: -2719.008264462809
     Maximum View E: 4261.767876392383
     Extent Method: Manual
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
