NOTE 15301:  Began computing simulation run "BUWO" at time 18Jul2024, 10:15:43.
NOTE 20364:  Found no parameter problems in meteorologic model "U-1-A".
WARNING 43652:  Sediment transport method has not been set for basin "Urban WS".
NOTE 40049:  Found no parameter problems in basin model "Urban WS".
WARNING 20657:  Hyetograph gage "U-1-A" for subbasin "U-1" contains 11020 missing or negative precipitation values that were set to zero.
NOTE 41959:  Clark parameters used to produce unit hydrograph for subbasin "U-1" are Tc=0.1818 R=1.0551
NOTE 42413:  Unit hydrograph volume for subbasin "U-1" is 1.0000 in.
NOTE 43212:  2 events above flow-rate threshold, 0.039, for subbasin "U-1".
NOTE 15302:  Finished computing simulation run "BUWO" at time 18Jul2024, 10:15:43.
NOTE 15312:  The total runtime for this simulation is 00:00.
