Meteorology: Dec_2005
     Description: Dec 2005 event; temperature index
     Last Modified Date: 21 June 2019
     Last Modified Time: 22:36:34
     Version: 4.5
     Unit System: English
     Set Missing Data to Default: Yes
     Precipitation Method: Gridded Precipitation
     Short-Wave Radiation Method: None
     Long-Wave Radiation Method: None
     Snowmelt Method: Gridded Temperature Index
     Evapotranspiration Method: Gridded Hamon
     Use Basin Model: Dec_2005
End:

Precip Method Parameters: Gridded Precipitation
     Last Modified Date: 21 June 2019
     Last Modified Time: 22:33:59
     Precip Grid Name: Dec_2005_gageInterp
End:

Snow Method Parameters: Gridded Temperature Index
     Last Modified Date: 21 June 2019
     Last Modified Time: 22:34:06
     Temperature Grid Name: Dec_2005_gageInterp
End:

Evapotranspiration Method Parameters: Gridded Hamon
     Last Modified Date: 21 June 2019
     Last Modified Time: 22:34:02
     Air Temperature Grid Name: Dec_2005_gageInterp
     Hamon Coefficient: 0.0065
End:

Subbasin: UpTruckeeRv_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34.5
     Snow vs Rain Temperature: 34.5
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Echo_Peak
     Melt Rate ATI-Melt Rate Table Name: Hagans_Meadow
     End Snow:
End:

Subbasin: TroutCk_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 33
     Snow vs Rain Temperature: 35
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Heavenly_Valley_slower
     End Snow:
End:

Subbasin: LakeTahoe_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S100
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: DonnerCk_S20
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 36
     Snow vs Rain Temperature: 37
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Earlier
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak_slower
     End Snow:
End:

Subbasin: DonnerCk_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: MartisCk_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak_slower_2
     End Snow:
End:

Subbasin: TruckeeRv_S90
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: ProsserCk_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 36
     Snow vs Rain Temperature: 36
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: LtTruckeeRv_S30
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak_slower_2
     End Snow:
End:

Subbasin: LtTruckeeRv_S20
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 33.5
     Snow vs Rain Temperature: 33.5
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: LtTruckeeRv_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 33
     Snow vs Rain Temperature: 33
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S80
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S70
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 35
     Snow vs Rain Temperature: 35
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Mt_Rose_Ski_Area_slower
     End Snow:
End:

Subbasin: DogCk_S10
     Last Modified Date: 15 August 2019
     Last Modified Time: 17:54:11

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 31
     Snow vs Rain Temperature: 31
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S60
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Mt_Rose_Ski_Area_slower
     End Snow:
End:

Subbasin: TruckeeRv_S50
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 33
     Snow vs Rain Temperature: 33
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Mt_Rose_Ski_Area_slower
     End Snow:
End:

Subbasin: TruckeeRv_S40
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 30
     Snow vs Rain Temperature: 30
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Mt_Rose_Ski_Area_much_slower
     End Snow:
End:

Subbasin: NTruckeeDt_S20
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 32
     Snow vs Rain Temperature: 32
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: NTruckeeDt_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 32
     Snow vs Rain Temperature: 32
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S30
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 32
     Snow vs Rain Temperature: 32
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: SteamboatCk_S40
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: SteamboatCk_S30
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: SteamboatCk_S20
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 34
     Snow vs Rain Temperature: 34
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: SteamboatCk_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 31
     Snow vs Rain Temperature: 31
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S20
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 32
     Snow vs Rain Temperature: 32
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:

Subbasin: TruckeeRv_S10
     Last Modified Date: 7 August 2020
     Last Modified Time: 23:10:21

     Begin Snow:
     Temperature Grid Name: Jan_1997_gageInterp

     Use Default Initial Values: No
     Cold Content Grid Name: Dec_2005_CC
     Cold Content ATI Grid Name: zeroCCATI
     Liquid Water Grid Name: zeroLWC
     Melt Rate ATI Grid Name: zeroMRATI
     Snow Water Equivalent Grid Name: Dec_2005_iSWE

     Base Temperature: 32
     Snow vs Rain Temperature: 32
     Dry Melt Rain Rate Limit: 0.1
     Cold Content ATI Snow Rate Limit: 0.2
     Cold Content ATI Decay Factor: 0.35
     Melt Rate ATI Decay Factor: 0.98
     Tree Line Elevation: 10000
     Interception Capacity: 0.0
     Liquid Water Holding Capacity: 3
     Ground Melt Method: Fixed Value
     Ground Melt Rate: 0
     Dry Melt Rate Method: ATI Function
     Wet Melt Method: Fixed Value
     Rain Melt Rate: 0.1

     Melt Rate ATI-Cold Rate Table Name: Averaged
     Melt Rate ATI-Melt Rate Table Name: Echo_Peak
     End Snow:
End:
