Basin: WY2017_local_obs
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:07:41
     Version: 4.5
     Filepath Separator: \
     Unit System: English
     Grid Region Name: Truckee_River
     Missing Flow To Zero: Yes
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: Yes

     Enable Sediment Routing: No

     Enable Quality Routing: No
End:

Source: Vista_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:02:01
     Canvas X: -6553581.787379821
     Canvas Y: 6833473.308471885
     From Canvas X: -6553581.787379821
     From Canvas Y: 6833473.308471885
     Downstream: TruckeeRv_R20

     Flow Method: GAGE_FLOW
     Flow Gage: Vista
     End Flow Method:
End:

Reach: TruckeeRv_R20
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:01:47
     Canvas X: -6512400.0
     Canvas Y: 6839020.0
     From Canvas X: -6555690.0
     From Canvas Y: 6836310.0
     Downstream: Tracy

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 56966
     Energy Slope: 0.0019
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: TruckeeRv_R20
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: Tracy
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6512400.0
     Canvas Y: 6839020.0
     Computation Point: Yes
     Observed Hydrograph Gage: Tracy
     Downstream: Tracy_SINK
End:

Sink: Tracy_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:04:31
     Canvas X: -6509365.341025368
     Canvas Y: 6835302.717382821
     From Canvas X: -6509365.341025368
     From Canvas Y: 6835302.717382821
End:

Source: Tracy_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:04:43
     Canvas X: -6513771.360132783
     Canvas Y: 6842336.88823853
     From Canvas X: -6513771.360132783
     From Canvas Y: 6842336.88823853
     Downstream: TruckeeRv_R10

     Flow Method: GAGE_FLOW
     Flow Gage: Tracy
     End Flow Method:
End:

Reach: TruckeeRv_R10
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:04:36
     Canvas X: -6482110.0
     Canvas Y: 6842630.0
     From Canvas X: -6512400.0
     From Canvas Y: 6839020.0
     Downstream: DerbyDam_IN

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 41857
     Energy Slope: 0.0017
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: TruckeeRv_R10
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: DerbyDam_IN
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6482110.0
     Canvas Y: 6842630.0
     Computation Point: Yes
     Observed Hydrograph Gage: DerbyDam_IN
End:

Source: Steamboat_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:04:07
     Canvas X: -6580857.828762567
     Canvas Y: 6786987.783990794
     From Canvas X: -6580857.828762567
     From Canvas Y: 6786987.783990794
     Downstream: SteamboatCk_R20

     Flow Method: GAGE_FLOW
     Flow Gage: Steamboat
     End Flow Method:
End:

Reach: SteamboatCk_R20
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:03:29
     Canvas X: -6568110.0
     Canvas Y: 6818710.0
     From Canvas X: -6580270.0
     From Canvas Y: 6788190.0
     Downstream: ShortLane

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 41978
     Energy Slope: 0.0045
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: SteamboatCk_R20
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: ShortLane
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6568110.0
     Canvas Y: 6818710.0
     Computation Point: Yes
     Observed Hydrograph Gage: ShortLane
     Downstream: ShortLane_SINK
End:

Sink: ShortLane_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:02:29
     Canvas X: -6566158.737444946
     Canvas Y: 6817243.053864024
     From Canvas X: -6566158.737444946
     From Canvas Y: 6817243.053864024
End:

Source: BocaBridge_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:57:03
     Canvas X: -6671244.899648108
     Canvas Y: 6813929.779600895
     From Canvas X: -6671244.899648108
     From Canvas Y: 6813929.779600895
     Downstream: TruckeeRv_R70

     Flow Method: GAGE_FLOW
     Flow Gage: BocaBridge
     End Flow Method:
End:

Reach: TruckeeRv_R70
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:56:47
     Canvas X: -6654370.0
     Canvas Y: 6826510.0
     From Canvas X: -6674670.0
     From Canvas Y: 6815190.0
     Downstream: Farad

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R70
     Channel Loss: None
End:

Junction: Farad
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6654370.0
     Canvas Y: 6826510.0
     Computation Point: Yes
     Observed Hydrograph Gage: Farad
     Downstream: Farad_SINK
End:

Sink: Farad_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:57:22
     Canvas X: -6656931.132669223
     Canvas Y: 6827405.083242112
     From Canvas X: -6656931.132669223
     From Canvas Y: 6827405.083242112
End:

Source: Mogul_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:58:43
     Canvas X: -6618242.038659349
     Canvas Y: 6849804.032405712
     From Canvas X: -6618242.038659349
     From Canvas Y: 6849804.032405712
     Downstream: TruckeeRv_R40

     Flow Method: GAGE_FLOW
     Flow Gage: Mogul
     End Flow Method:
End:

Reach: TruckeeRv_R40
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:58:33
     Canvas X: -6580340.0
     Canvas Y: 6846210.0
     From Canvas X: -6619560.0
     From Canvas Y: 6847610.0
     Downstream: Reno

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R40
     Channel Loss: None
End:

Junction: Reno
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6580340.0
     Canvas Y: 6846210.0
     Computation Point: Yes
     Observed Hydrograph Gage: Reno
     Downstream: Reno_SINK
End:

Sink: Reno_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:59:02
     Canvas X: -6581229.871324822
     Canvas Y: 6843335.886657954
     From Canvas X: -6581229.871324822
     From Canvas Y: 6843335.886657954
End:

Source: ShortLane_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:02:44
     Canvas X: -6570291.163894913
     Canvas Y: 6820297.456022713
     From Canvas X: -6570291.163894913
     From Canvas Y: 6820297.456022713
     Downstream: SteamboatCk_R10

     Flow Method: GAGE_FLOW
     Flow Gage: ShortLane
     End Flow Method:
End:

Reach: SteamboatCk_R10
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:40:32
     Canvas X: -6559450.0
     Canvas Y: 6834420.0
     From Canvas X: -6568110.0
     From Canvas Y: 6818710.0
     Downstream: Cleanwater

     Route: Lag
     Initial Variable: Combined Inflow
     Lag: 60
     Channel Loss: None
End:

Junction: Cleanwater
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6559450.0
     Canvas Y: 6834420.0
     Computation Point: Yes
     Observed Hydrograph Gage: Cleanwater
     Downstream: Cleanwater_SINK
End:

Sink: Cleanwater_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:01:07
     Canvas X: -6565739.505776117
     Canvas Y: 6834072.210855926
     From Canvas X: -6565739.505776117
     From Canvas Y: 6834072.210855926
End:

Source: Farad_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:57:34
     Canvas X: -6651121.779543903
     Canvas Y: 6827225.412526891
     From Canvas X: -6651121.779543903
     From Canvas Y: 6827225.412526891
     Downstream: TruckeeRv_R60

     Flow Method: GAGE_FLOW
     Flow Gage: Farad
     End Flow Method:
End:

Reach: TruckeeRv_R60
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:57:26
     Canvas X: -6634720.0
     Canvas Y: 6857920.0
     From Canvas X: -6654370.0
     From Canvas Y: 6826510.0
     Downstream: DogCk_CF

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R60
     Channel Loss: None
End:

Source: DogCreek_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:58:10
     Canvas X: -6636628.341849804
     Canvas Y: 6859985.372934626
     From Canvas X: -6636628.341849804
     From Canvas Y: 6859985.372934626
     Downstream: DogCk_CF

     Flow Method: GAGE_FLOW
     Flow Gage: DogCreek
     End Flow Method:
End:

Junction: DogCk_CF
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6634720.0
     Canvas Y: 6857920.0
     Downstream: TruckeeRv_R50
End:

Reach: TruckeeRv_R50
     Last Modified Date: 6 March 2019
     Last Modified Time: 05:18:10
     Canvas X: -6619560.0
     Canvas Y: 6847610.0
     From Canvas X: -6634720.0
     From Canvas Y: 6857920.0
     Downstream: Mogul

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R50
     Channel Loss: None
End:

Junction: Mogul
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6619560.0
     Canvas Y: 6847610.0
     Computation Point: Yes
     Observed Hydrograph Gage: Mogul
     Downstream: Mogul_SINK
End:

Sink: Mogul_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:58:28
     Canvas X: -6619859.075096295
     Canvas Y: 6844653.471902849
     From Canvas X: -6619859.075096295
     From Canvas Y: 6844653.471902849
End:

Source: TahoeCity_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:46:01
     Canvas X: -6706914.172533611
     Canvas Y: 6738316.184527628
     From Canvas X: -6706914.172533611
     From Canvas Y: 6738316.184527628
     Downstream: TruckeeRv_R100

     Flow Method: GAGE_FLOW
     Flow Gage: TahoeCity
     End Flow Method:
End:

Reach: TruckeeRv_R100
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:45:52
     Canvas X: -6712990.0
     Canvas Y: 6791700.0
     From Canvas X: -6708250.0
     From Canvas Y: 6741380.0
     Downstream: Truckee

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 74300
     Energy Slope: 0.0053
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: TruckeeRv_R100
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: Truckee
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6712990.0
     Canvas Y: 6791700.0
     Computation Point: Yes
     Observed Hydrograph Gage: Truckee
     Downstream: Truckee_SINK
End:

Sink: Truckee_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:46:27
     Canvas X: -6717399.260090672
     Canvas Y: 6792632.375806818
     From Canvas X: -6717399.260090672
     From Canvas Y: 6792632.375806818
End:

Source: Reno_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:59:15
     Canvas X: -6579433.1641726615
     Canvas Y: 6848426.556922401
     From Canvas X: -6579433.1641726615
     From Canvas Y: 6848426.556922401
     Downstream: TruckeeRv_R30

     Flow Method: GAGE_FLOW
     Flow Gage: Reno
     End Flow Method:
End:

Reach: TruckeeRv_R30
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:59:08
     Canvas X: -6556900.0
     Canvas Y: 6836890.0
     From Canvas X: -6580340.0
     From Canvas Y: 6846210.0
     Downstream: NTruckeeDt_CF

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 31331
     Energy Slope: 0.0021
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: TruckeeRv_R30
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Source: BigFishDrive_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:00:44
     Canvas X: -6551605.409512442
     Canvas Y: 6842935.966139936
     From Canvas X: -6551605.409512442
     From Canvas Y: 6842935.966139936
     Downstream: NTruckeeDt_CF

     Flow Method: GAGE_FLOW
     Flow Gage: BigFishDrive
     End Flow Method:
End:

Junction: NTruckeeDt_CF
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6556900.0
     Canvas Y: 6836890.0
     Downstream: Vista
End:

Source: Cleanwater_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:01:55
     Canvas X: -6557714.21382979
     Canvas Y: 6832395.284180583
     From Canvas X: -6557714.21382979
     From Canvas Y: 6832395.284180583
     Downstream: Vista

     Flow Method: GAGE_FLOW
     Flow Gage: Cleanwater
     End Flow Method:
End:

Junction: Vista
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6555690.0
     Canvas Y: 6836310.0
     Computation Point: Yes
     Observed Hydrograph Gage: Vista
     Downstream: Vista_SINK
End:

Sink: Vista_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:01:42
     Canvas X: -6552863.10451896
     Canvas Y: 6838563.978736327
     From Canvas X: -6552863.10451896
     From Canvas Y: 6838563.978736327
End:

Source: abBocaDam_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:54:04
     Canvas X: -6666120.906121317
     Canvas Y: 6830987.559105455
     From Canvas X: -6666120.906121317
     From Canvas Y: 6830987.559105455
     Downstream: LtTruckeeRv_R10

     Flow Method: GAGE_FLOW
     Flow Gage: abBocaDam
     End Flow Method:
End:

Reach: LtTruckeeRv_R10
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:52:59
     Canvas X: -6673559.045266732
     Canvas Y: 6819850.16045951
     From Canvas X: -6667320.0
     From Canvas Y: 6832820.0
     Downstream: Boca_IN

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 21713
     Energy Slope: 0.0054
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: LtTruckeeRv_R10
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: Boca_IN
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6673559.045266732
     Canvas Y: 6819850.16045951
     Computation Point: Yes
     Observed Hydrograph Gage: Boca_IN
     Downstream: Boca_SINK
End:

Sink: Boca_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:51:53
     Canvas X: -6675904.907749251
     Canvas Y: 6819135.436883023
     From Canvas X: -6675904.907749251
     From Canvas Y: 6819135.436883023
End:

Source: blDonnerDam_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 18:14:48
     Canvas X: -6719935.188525975
     Canvas Y: 6805451.168295115
     From Canvas X: -6719935.188525975
     From Canvas Y: 6805451.168295115
     Downstream: DonnerCk_R10

     Flow Method: GAGE_FLOW
     Flow Gage: blDonnerDam
     End Flow Method:
End:

Reach: DonnerCk_R10
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:47:06
     Canvas X: -6711380.0
     Canvas Y: 6800680.0
     From Canvas X: -6718300.0
     From Canvas Y: 6803430.0
     Downstream: Hwy89

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 14556
     Energy Slope: 0.0070
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: DonnerCk_R10
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: Hwy89
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:35
     Canvas X: -6711380.0
     Canvas Y: 6800680.0
     Computation Point: Yes
     Observed Hydrograph Gage: Hwy89
     Downstream: Hwy89_SINK
End:

Sink: Hwy89_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:47:34
     Canvas X: -6712949.232155676
     Canvas Y: 6799257.726539128
     From Canvas X: -6712949.232155676
     From Canvas Y: 6799257.726539128
End:

Source: MartisCreek_OUT_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:48:23
     Canvas X: -6684491.588580397
     Canvas Y: 6795133.430368801
     From Canvas X: -6684491.588580397
     From Canvas Y: 6795133.430368801
     Downstream: MartisCk_R10

     Flow Method: GAGE_FLOW
     Flow Gage: MartisCreek_OUT
     End Flow Method:
End:

Reach: MartisCk_R10
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:48:14
     Canvas X: -6684470.117727125
     Canvas Y: 6804452.656369946
     From Canvas X: -6685360.0
     From Canvas Y: 6796320.0
     Downstream: blMartisCreekDam

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: MartisCk_R10
     Channel Loss: None
End:

Source: Truckee_SOURCE
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:34:37
     Canvas X: -6711383.226246458
     Canvas Y: 6794093.412597571
     From Canvas X: -6711383.226246458
     From Canvas Y: 6794093.412597571
     Downstream: DonnerCk_CF

     Flow Method: GAGE_FLOW
     Flow Gage: Truckee
     End Flow Method:
End:

Source: Hwy89_SOURCE
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:34:41
     Canvas X: -6708733.284959342
     Canvas Y: 6801961.431806343
     From Canvas X: -6708733.284959342
     From Canvas Y: 6801961.431806343
     Downstream: DonnerCk_CF

     Flow Method: GAGE_FLOW
     Flow Gage: Hwy89
     End Flow Method:
End:

Junction: DonnerCk_CF
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:34:41
     Canvas X: -6709800.0
     Canvas Y: 6798440.0
     Downstream: TruckeeRv_R90
End:

Reach: TruckeeRv_R90
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:38:28
     Canvas X: -6684470.117727125
     Canvas Y: 6804452.656369946
     From Canvas X: -6709800.0
     From Canvas Y: 6798440.0
     Downstream: blMartisCreekDam

     Route: Lag
     Initial Variable: Combined Inflow
     Lag: 60
     Channel Loss: None
End:

Junction: blMartisCreekDam
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:30:53
     Canvas X: -6684470.117727125
     Canvas Y: 6804452.656369946
     From Canvas X: -6684470.117727125
     From Canvas Y: 6804452.656369946
     Computation Point: Yes
     Observed Hydrograph Gage: blMartisCreekDam
     Downstream: blMartisCreekDam_SINK
End:

Sink: blMartisCreekDam_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:48:51
     Canvas X: -6681742.05780018
     Canvas Y: 6804069.405404508
     From Canvas X: -6681742.05780018
     From Canvas Y: 6804069.405404508
End:

Source: SpanishSprings_SOUCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:00:02
     Canvas X: -6559271.36002833
     Canvas Y: 6857309.623357219
     From Canvas X: -6559271.36002833
     From Canvas Y: 6857309.623357219
     Downstream: NTruckeeDt_R10

     Flow Method: GAGE_FLOW
     Flow Gage: SpanishSprings
     End Flow Method:
End:

Reach: NTruckeeDt_R10
     Last Modified Date: 26 April 2019
     Last Modified Time: 05:40:45
     Canvas X: -6558460.0
     Canvas Y: 6841230.0
     From Canvas X: -6559058.463337679
     From Canvas Y: 6854451.536662321
     Downstream: BigFishDrive

     Route: Lag
     Initial Variable: Combined Inflow
     Lag: 60
     Channel Loss: None
End:

Junction: BigFishDrive
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6558460.0
     Canvas Y: 6841230.0
     Computation Point: Yes
     Observed Hydrograph Gage: BigFishDrive
     Downstream: BigFishDrive_SINK
End:

Sink: BigFishDrive_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:00:32
     Canvas X: -6561966.420756574
     Canvas Y: 6844553.002576877
     From Canvas X: -6561966.420756574
     From Canvas Y: 6844553.002576877
End:

Source: blProsserCreek_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:49:49
     Canvas X: -6687498.762539178
     Canvas Y: 6815056.966225702
     From Canvas X: -6687498.762539178
     From Canvas Y: 6815056.966225702
     Downstream: ProsserCk_R10

     Flow Method: GAGE_FLOW
     Flow Gage: blProsserDam
     End Flow Method:
End:

Reach: ProsserCk_R10
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:49:49
     Canvas X: -6682040.0
     Canvas Y: 6811830.0
     From Canvas X: -6685830.0
     From Canvas Y: 6813880.0
     Downstream: ProsserCk_CF

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 8173
     Energy Slope: 0.0262
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: ProsserCk_R10
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Source: blMartisCreekDam_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:49:10
     Canvas X: -6686645.38769157
     Canvas Y: 6806452.3320807135
     From Canvas X: -6686645.38769157
     From Canvas Y: 6806452.3320807135
     Downstream: TruckeeRv_R85

     Flow Method: GAGE_FLOW
     Flow Gage: blMartisCreekDam
     End Flow Method:
End:

Reach: TruckeeRv_R85
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:48:55
     Canvas X: -6682040.0
     Canvas Y: 6811830.0
     From Canvas X: -6684470.117727125
     From Canvas Y: 6804452.656369946
     Downstream: ProsserCk_CF

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R85
     Channel Loss: None
End:

Junction: ProsserCk_CF
     Last Modified Date: 28 March 2018
     Last Modified Time: 12:00:00
     Canvas X: -6682040.0
     Canvas Y: 6811830.0
     Downstream: TruckeeRv_R80
End:

Reach: TruckeeRv_R80
     Last Modified Date: 6 March 2019
     Last Modified Time: 05:17:35
     Canvas X: -6674670.0
     Canvas Y: 6815190.0
     From Canvas X: -6682040.0
     From Canvas Y: 6811830.0
     Downstream: BocaBridge

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: TruckeeRv_R80
     Channel Loss: None
End:

Source: blBocaDam_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:52:26
     Canvas X: -6673063.725943021
     Canvas Y: 6817806.497005928
     From Canvas X: -6673063.725943021
     From Canvas Y: 6817806.497005928
     Downstream: BocaBridge

     Flow Method: GAGE_FLOW
     Flow Gage: blBocaDam
     End Flow Method:
End:

Junction: BocaBridge
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:45
     Canvas X: -6674670.0
     Canvas Y: 6815190.0
     Computation Point: Yes
     Observed Hydrograph Gage: BocaBridge
     Downstream: BocaBridge_SINK
End:

Sink: BocaBridge_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:56:41
     Canvas X: -6672083.362985779
     Canvas Y: 6812432.5236407835
     From Canvas X: -6672083.362985779
     From Canvas Y: 6812432.5236407835
End:

Source: Stampede_OUT_SOURCE
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:56:07
     Canvas X: -6670705.8875024645
     Canvas Y: 6847767.764299931
     From Canvas X: -6670705.8875024645
     From Canvas Y: 6847767.764299931
     Downstream: LtTruckeeRv_R20

     Flow Method: GAGE_FLOW
     Flow Gage: StampedeDam_OUT
     End Flow Method:
End:

Reach: LtTruckeeRv_R20
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:55:55
     Canvas X: -6667320.0
     Canvas Y: 6832820.0
     From Canvas X: -6669410.0
     From Canvas Y: 6846550.0
     Downstream: abBocaDam

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 20817
     Energy Slope: 0.0173
     Mannings n: 0.035
     Left Mannings n: 0.075
     Right Mannings n: 0.075
     Cross Section Name: LtTruckeeRv_R20
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: abBocaDam
     Last Modified Date: 25 April 2019
     Last Modified Time: 04:06:54
     Canvas X: -6667320.0
     Canvas Y: 6832820.0
     Computation Point: Yes
     Observed Hydrograph Gage: abBocaDam
     Downstream: abBocaDam_SINK
End:

Sink: abBocaDam_SINK
     Last Modified Date: 25 April 2019
     Last Modified Time: 03:52:55
     Canvas X: -6671211.576385778
     Canvas Y: 6832604.595542405
     From Canvas X: -6671211.576385778
     From Canvas Y: 6832604.595542405
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     Element Layer:
          Name: Reaches
          Layer shown: Yes
     End Layer:
     Element Layer:
          Name: Subbasins
          Layer shown: Yes
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["GCS_North_American_1983",DATUM["North_American_Datum_1983",SPHEROID["GRS_1980",6378137.0,298.257222101]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["False_Easting",0.0],PARAMETER["False_Northing",0.0],PARAMETER["longitude_of_center",-96.0],PARAMETER["Standard_Parallel_1",29.5],PARAMETER["Standard_Parallel_2",45.5],PARAMETER["latitude_of_center",23.0],UNIT["Foot_US",0.3048006096012192]]
End:

Basin Schematic Properties:
     Last View N: 6921432.5362358475
     Last View S: 6763659.615044729
     Last View W: -6749790.905608622
     Last View E: -6618204.361378685
     Maximum View N: 6893191.186775439
     Maximum View S: 6592254.732971415
     Maximum View W: -6746583.735067542
     Maximum View E: -6469516.012615832
     Extent Method: Elements
     Buffer: 10
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: Yes
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Default
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: Yes
     Fix Hydrologic Order: No
End:

Computation Point: Tracy
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: DerbyDam_IN
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: ShortLane
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Farad
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Reno
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Cleanwater
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Mogul
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Truckee
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Vista
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Boca_IN
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Hwy89
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: blMartisCreekDam
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: BigFishDrive
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: BocaBridge
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: abBocaDam
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 
