NOTE 15301:  Began computing simulation run "MSDPM_SDR_M" at time 03Nov2025, 06:42:06.
NOTE 20364:  Found no parameter problems in meteorologic model "2003_Event".
WARNING 49903:  Cohesive sediment transport method has not been set for reach "Reach-1".
NOTE 40049:  Found no parameter problems in basin model "Deer_Ck_DB_MSDPM_SDR-M".
NOTE 41089:  Routing parameters based on index flow 20.0 m3/s for reach "Reach-1": Delta t (sec) 60.0  Delta x (m) 398.5813
NOTE 41102:  Index flow 20.0 (m3/s) for reach "Reach-1" translates to an index celerity of 7.22 (m/s).
WARNING 20657:  Hyetograph gage "Mt. Baldy (MTBY)" for subbasin "S_1" contains 857 missing or negative precipitation values that were set to zero.
WARNING 20657:  Hyetograph gage "Mt. Baldy (MTBY)" for subbasin "S_2" contains 857 missing or negative precipitation values that were set to zero.
WARNING 20657:  Hyetograph gage "Mt. Baldy (MTBY)" for subbasin "S_3" contains 857 missing or negative precipitation values that were set to zero.
NOTE 42413:  Unit hydrograph volume for subbasin "S_1" is 1.0000 mm.
NOTE 42413:  Unit hydrograph volume for subbasin "S_2" is 1.0000 mm.
NOTE 42413:  Unit hydrograph volume for subbasin "S_3" is 1.0000 mm.
NOTE 41079:  Routing incremental distance for reach "Reach-1" is based on specified index flow 20 m3/s.  Calculated index flow from minimum (0.0) and maximum (34.8) inflow is 17 m3/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 17 m3/s at reach "Reach-1" would have increased spatial steps from 8 to 15.
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Clay" 
	Bed load change: 0 	Suspended load change: 0 
	Inflow load: 0 	Outflow load: 0 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Silt" 
	Bed load change: 0 	Suspended load change: 0 
	Inflow load: 0 	Outflow load: 0 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Sand" 
	Bed load change: 0 	Suspended load change: 0 
	Inflow load: 0 	Outflow load: 0 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Gravel" 
	Bed load change: 0 	Suspended load change: 0 
	Inflow load: 0 	Outflow load: 0 
	Net error: 0 tonnes
NOTE 41079:  Routing incremental distance for reach "Reach-1" is based on specified index flow 20 m3/s.  Calculated index flow from minimum (0.0) and maximum (34.8) inflow is 17 m3/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 17 m3/s at reach "Reach-1" would have increased spatial steps from 8 to 15.
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Clay" 
	Bed load change: 0 	Suspended load change: 0 
	Inflow load: 0 	Outflow load: 0 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Silt" 
	Bed load change: 566.244 	Suspended load change: 0 
	Inflow load: 1,718.161 	Outflow load: 1,151.917 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Sand" 
	Bed load change: 12,082.582 	Suspended load change: 0 
	Inflow load: 26,368.719 	Outflow load: 14,286.136 
	Net error: 0 tonnes
NOTE 43514:  Sediment continuity check for reach "Reach-1", grade: "Gravel" 
	Bed load change: 63,445.621 	Suspended load change: 0 
	Inflow load: 112,347.517 	Outflow load: 48,901.896 
	Net error: 0 tonnes
NOTE 15302:  Finished computing simulation run "MSDPM_SDR_M" at time 03Nov2025, 06:42:47.
NOTE 15312:  The total runtime for this simulation is 00:41.
