Basin: Deer_Ck_DB_MSDPM
     Last Modified Date: 3 November 2022
     Last Modified Time: 21:25:32
     Version: 4.14
     Filepath Separator: \
     Unit System: Metric
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: Yes
     Sediment Grade Scale: SIMPLE_4
     Sediment Properties: 
     Sediment Specific Gravity: 2.65
     Unit Weight Sand Gravel: 1487.7
     Unit Weight Silt: 1041.2
     Unit Weight Clay: 480.55
     End Sediment Properties: 
End:

Subbasin: Subbasin-1
     Last Modified Date: 4 April 2023
     Last Modified Time: 20:31:34
     Latitude Degrees:  34.19721313406235
     Longitude Degrees: -117.57901976714122
     Canvas X: -1956741.651805896
     Canvas Y: 1460135.7903467591
     Area: 9.7007
     Downstream: Sink-1

     Discretization: None
     File: Deer_Ck_DB_MSDPM.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.7
     Storage Coefficient: 0.7
     Time Area Method: Default

     Baseflow: None

     Sediment Erosion: Yes
     Erosion: MSDPM
     Gradation Curve Name: Debris Flow Mixture
     Sediment Concentration Exponent: 1
     Fire Factor Type: Pak & Lee
     Fire Factor: 6.5
     Transposition Factor: 1.0
     Minimum Rainfall: 24.32
     Rainfall Intensity Threshold: 8.771
     Relief Ratio: 233.20
     Percent Burn: 100
     Erosion Flow Rate Threshold: 32
     Burn Date: 15 October 2003
     End Erosion:
End:

Sink: Sink-1
     Last Modified Date: 3 November 2022
     Last Modified Time: 17:16:00
     Canvas X: -1956366.3416842762
     Canvas Y: 1457484.7595348505
     From Canvas X: -1956255.741889656
     From Canvas Y: 1456466.5311504558
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     Element Layer:
          Name: Reaches
          Layer shown: Yes
     End Layer:
     2D Connection Layer:
          Layer shown: No
     End Layer:
     Element Layer:
          Name: Subbasins
          Layer shown: Yes
     End Layer:
     Discretization Layer:
          Layer shown: No
     End Layer:
     Breakpoint Layer:
          Layer shown: Yes
     End Layer:
     Base Layer:
          Name: Identified Streams
          Layer shown: Yes
          Properties Filename: maps\streams1453132912023.xml
     End Layer:
     Base Layer:
          Name: Flow Accumulation
          Layer shown: No
          Properties Filename: maps\flowaccum1453132912023.xml
     End Layer:
     Base Layer:
          Name: Flow Direction
          Layer shown: No
          Properties Filename: maps\flowdir1453132912023.xml
     End Layer:
     Base Layer:
          Name: Sink Locations
          Layer shown: No
          Properties Filename: maps\sinklocs1453132912023.xml
     End Layer:
     Base Layer:
          Name: Sink Fill
          Layer shown: No
          Properties Filename: maps\sinkfill1453132912023.xml
     End Layer:
     Base Layer:
          Name: Terrain
          Layer shown: Yes
          Properties Filename: maps\elevation3125143072022.xml
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["NAD83",DATUM["North_American_Datum_1983",SPHEROID["GRS 1980",6378137,298.257222101004,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","6269"]],PRIMEM["Greenwich",0],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4269"]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["latitude_of_center",23],PARAMETER["longitude_of_center",-96],PARAMETER["standard_parallel_1",29.5],PARAMETER["standard_parallel_2",45.5],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH]]
     Terrain: NED_10m
     Threshold: 1
     Break Point: Break Point 1
          X Coordinate: -1956437.9597804511
          Y Coordinate: 1457394.3334884408
     End Break Point:
     reach_prefix: R_
     junction_insert: true
     junction_prefix: J_
     subbasin_prefix: S_
End:

Basin Schematic Properties:
     Last View N: 1461266.2308844957
     Last View S: 1457396.0591359593
     Last View W: -1957239.430230012
     Last View E: -1956339.2088152347
     Maximum View N: 1460135.7903467591
     Maximum View S: 1457484.7595348505
     Maximum View W: -1956741.651805896
     Maximum View E: -1956366.3416842762
     Extent Method: Elements
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
