Basin: Deer_Ck_DB_MSDPM_SDR-M
     Last Modified Date: 8 November 2022
     Last Modified Time: 21:33:02
     Version: 4.14
     Filepath Separator: \
     Unit System: Metric
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: Yes
     Sediment Grade Scale: SIMPLE_4
     Sediment Properties: 
     Sediment Specific Gravity: 2.65
     Unit Weight Sand Gravel: 1489.7
     Unit Weight Silt: 1041.2
     Unit Weight Clay: 480.55
     End Sediment Properties: 
End:

Subbasin: S_1
     Last Modified Date: 4 April 2023
     Last Modified Time: 21:46:41
     Latitude Degrees:  34.20606333332723
     Longitude Degrees: -117.58710588695972
     Canvas X: -1957239.430230012
     Canvas Y: 1461266.2308844957
     Area: 2.5647
     Downstream: J_2

     Discretization: None
     File: Deer_Ck_DB_MSDPM_SDR_M.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.5
     Storage Coefficient: 0.5
     Time Area Method: Default

     Baseflow: None

     Sediment Erosion: Yes
     Erosion: MSDPM
     Gradation Curve Name: Debris Flow Mixture
     Sediment Concentration Exponent: 1
     Fire Factor Type: Pak & Lee
     Transposition Factor: 1.0
     Minimum Rainfall: 20.665
     Rainfall Intensity Threshold: 6.8163
     Relief Ratio: 369.09
     Percent Burn: 100
     Erosion Flow Rate Threshold: 0.030
     Burn Date: 15 October 2003
     End Erosion:
End:

Subbasin: S_2
     Last Modified Date: 4 April 2023
     Last Modified Time: 21:47:03
     Latitude Degrees:  34.2050438130258
     Longitude Degrees: -117.57671485808645
     Canvas X: -1956339.2088152347
     Canvas Y: 1460941.2309194384
     Area: 2.5602
     Downstream: J_2

     Discretization: None
     File: Deer_Ck_DB_MSDPM_SDR_M.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.5
     Storage Coefficient: 0.5
     Time Area Method: Default

     Baseflow: None

     Sediment Erosion: Yes
     Erosion: MSDPM
     Gradation Curve Name: Debris Flow Mixture
     Sediment Concentration Exponent: 1
     Fire Factor Type: Pak & Lee
     Transposition Factor: 1.0
     Minimum Rainfall: 22.132
     Rainfall Intensity Threshold: 7.5787
     Relief Ratio: 304.28
     Percent Burn: 100
     Erosion Flow Rate Threshold: 0.030
     Burn Date: 15 October 2003
     End Erosion:
End:

Junction: J_2
     Last Modified Date: 3 November 2022
     Last Modified Time: 14:51:57
     Canvas X: -1956990.601378548
     Canvas Y: 1459464.1751465003
     Downstream: Reach-1
End:

Reach: Reach-1
     Last Modified Date: 4 April 2023
     Last Modified Time: 22:00:28
     Canvas X: -1956461.711044124
     Canvas Y: 1457419.0890730722
     From Canvas X: -1956990.601378548
     From Canvas Y: 1459464.1751465003
     Downstream: J_1

     Route: Muskingum Cunge
     Channel: Trapezoid
     Length: 3188.65
     Energy Slope: 0.12406
     Mannings n: 0.05
     Bottom Width: 1
     Side Slope: 0.5
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Flow
     Index Flow: 20
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None

     Route Sediment: Yes
     Sediment Transport Potential: Sediment Delivery Ratio
     Grain Type: Clay
     Sediment Delivery Ratio: 1.0
     End Grain Type: Clay
     Grain Type: Silt
     Sediment Delivery Ratio: 0.61
     End Grain Type: Silt
     Grain Type: Sand
     Sediment Delivery Ratio: 0.41
     End Grain Type: Sand
     Grain Type: Gravel
     Sediment Delivery Ratio: 0.21
     End Grain Type: Gravel
     Grain Type: Cobble
     End Grain Type: Cobble
     Grain Type: Boulder
     End Grain Type: Boulder
     End Sediment Transport Potential: Sediment Delivery Ratio
     Fall Velocity Method: van Rijn
     Hindered Settling Velocity: Clear Water
     End Settling Velocity:
     Sediment Bed Depth: 10
     Sediment Bed Width: 1
     Active Bed Depth Factor: 1
     Use Water Temperature Gage: No
     Average Water Temperature: 13.0
     Gradation Curve Name: Debris Flow Mixture
     Deposition Limit Method: --None--
     Erosion Limit Method: --NONE--
     Sediment Route Method: Muskingum Sediment Delivery
     Grain Type: Clay
     Sediment Attenuation Coefficient: 0.5
     Sediment Travel Time: 0.5
     End Grain Type: Clay
     Grain Type: Silt
     Sediment Attenuation Coefficient: 0.5
     Sediment Travel Time: 1
     End Grain Type: Silt
     Grain Type: Sand
     Sediment Attenuation Coefficient: 0.5
     Sediment Travel Time: 2
     End Grain Type: Sand
     Grain Type: Gravel
     Sediment Attenuation Coefficient: 0.5
     Sediment Travel Time: 5
     End Grain Type: Gravel
     Grain Type: Cobble
     End Grain Type: Cobble
     Grain Type: Boulder
     End Grain Type: Boulder
     End Sediment Router: Muskingum Sediment Delivery
End:

Subbasin: S_3
     Last Modified Date: 4 April 2023
     Last Modified Time: 21:46:54
     Latitude Degrees:  34.18787089488198
     Longitude Degrees: -117.57577799619773
     Canvas X: -1956687.8282239274
     Canvas Y: 1459051.5238640844
     Area: 4.5758
     Downstream: J_1

     Discretization: None
     File: Deer_Ck_DB_MSDPM_SDR_M.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 0.7
     Storage Coefficient: 0.7
     Time Area Method: Default

     Baseflow: None

     Sediment Erosion: Yes
     Erosion: MSDPM
     Gradation Curve Name: Debris Flow Mixture
     Sediment Concentration Exponent: 1
     Fire Factor Type: Pak & Lee
     Transposition Factor: 1.0
     Minimum Rainfall: 24.468
     Rainfall Intensity Threshold: 8.8514
     Relief Ratio: 229.35
     Percent Burn: 100
     Erosion Flow Rate Threshold: 0.030
     Burn Date: 15 October 2003
     End Erosion:
End:

Junction: J_1
     Last Modified Date: 4 November 2022
     Last Modified Time: 23:02:58
     Canvas X: -1956461.711044124
     Canvas Y: 1457419.0890730722
     From Canvas X: -1954879.5832971488
     From Canvas Y: 1457591.0594803598
     Downstream: Sink-1
End:

Sink: Sink-1
     Last Modified Date: 4 November 2022
     Last Modified Time: 18:39:31
     Canvas X: -1956340.754176945
     Canvas Y: 1456645.4892943974
     From Canvas X: -1956255.741889656
     From Canvas Y: 1456466.5311504558
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     Element Layer:
          Name: Reaches
          Layer shown: Yes
     End Layer:
     2D Connection Layer:
          Layer shown: No
     End Layer:
     Element Layer:
          Name: Subbasins
          Layer shown: Yes
     End Layer:
     Discretization Layer:
          Layer shown: No
     End Layer:
     Breakpoint Layer:
          Layer shown: Yes
     End Layer:
     Base Layer:
          Name: Identified Streams
          Layer shown: Yes
          Properties Filename: maps\streams2353132912023.xml
     End Layer:
     Base Layer:
          Name: Flow Accumulation
          Layer shown: No
          Properties Filename: maps\flowaccum2353132912023.xml
     End Layer:
     Base Layer:
          Name: Flow Direction
          Layer shown: No
          Properties Filename: maps\flowdir2353132912023.xml
     End Layer:
     Base Layer:
          Name: Sink Locations
          Layer shown: No
          Properties Filename: maps\sinklocs2353132912023.xml
     End Layer:
     Base Layer:
          Name: Sink Fill
          Layer shown: No
          Properties Filename: maps\sinkfill2353132912023.xml
     End Layer:
     Base Layer:
          Name: Terrain
          Layer shown: Yes
          Properties Filename: maps\elevation0233133122022.xml
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["NAD83",DATUM["North_American_Datum_1983",SPHEROID["GRS 1980",6378137,298.257222101004,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","6269"]],PRIMEM["Greenwich",0],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4269"]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["latitude_of_center",23],PARAMETER["longitude_of_center",-96],PARAMETER["standard_parallel_1",29.5],PARAMETER["standard_parallel_2",45.5],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH]]
     Terrain: NED_10m
     Threshold: 1
     Break Point: Break Point 1
          X Coordinate: -1956437.9597804511
          Y Coordinate: 1457394.3334884408
     End Break Point:
     reach_prefix: R_
     junction_insert: true
     junction_prefix: J_
     subbasin_prefix: S_
End:

Basin Schematic Properties:
     Last View N: 1461266.2308844957
     Last View S: 1457396.0591359593
     Last View W: -1957239.430230012
     Last View E: -1956339.2088152347
     Maximum View N: 1461266.2308844957
     Maximum View S: 1457396.0591359593
     Maximum View W: -1957239.430230012
     Maximum View E: -1956339.2088152347
     Extent Method: Elements
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
