NOTE 15301:  Began computing simulation run "Kanopolis E Chen Calib_ESAD" at time 22Jul2022, 14:25:04.
NOTE 20364:  Found no parameter problems in meteorologic model "Kanopolis".
WARNING 43652:  Sediment transport method has not been set for basin "Kanopolis_Chen_ESAD".
NOTE 10617:  Data type "INST-VAL" is usually used for time intervals less than 24 hours.  Gage "Kanopolis Inflow".
NOTE 10617:  Data type "INST-VAL" is usually used for time intervals less than 24 hours.  Gage "Kanopolis Elev".
NOTE 40049:  Found no parameter problems in basin model "Kanopolis_Chen_ESAD".
NOTE 10617:  Data type "INST-VAL" is usually used for time intervals less than 24 hours.  Gage "Kanopolis Elev".
WARNING 42176:  0 negative discharge values for source "Source-1".
NOTE 46852:  Sediment mass balance for reservoir "Kanopolis", grade: "Clay" 
	Bottom load change: 0.0 	Suspended load change: 0.0 
	Inflow load: 0.0 	Outflow load: 0.0 
	Net error: 0.0 tons
NOTE 46852:  Sediment mass balance for reservoir "Kanopolis", grade: "Silt" 
	Bottom load change: 0.0 	Suspended load change: 0.0 
	Inflow load: 0.0 	Outflow load: 0.0 
	Net error: 0.0 tons
NOTE 46852:  Sediment mass balance for reservoir "Kanopolis", grade: "Sand" 
	Bottom load change: 37,742,193.3 	Suspended load change: 0.0 
	Inflow load: 37,742,193.3 	Outflow load: 0.0 
	Net error: 0.0 tons
NOTE 46852:  Sediment mass balance for reservoir "Kanopolis", grade: "Gravel" 
	Bottom load change: 0.0 	Suspended load change: 0.0 
	Inflow load: 0.0 	Outflow load: 0.0 
	Net error: 0.0 tons
WARNING 41201:  3622 negative inflows to element "Kanopolis" set to zero.
     Equivalent volume (cu ft): -2,438,903,084.3473
NOTE 15302:  Finished computing simulation run "Kanopolis E Chen Calib_ESAD" at time 22Jul2022, 14:25:28.
NOTE 15312:  The total runtime for this simulation is 00:24.
