Basin: Big_Blue_R
     Last Modified Date: 10 May 2022
     Last Modified Time: 20:17:00
     Version: 4.10
     Filepath Separator: \
     Unit System: English
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: Yes
     Sediment Grade Scale: SIMPLE_4
     Sediment Properties: 
     Sediment Specific Gravity: 2.65
     Unit Weight Sand Gravel: 93
     Unit Weight Silt: 65
     Unit Weight Clay: 30
     End Sediment Properties: 
     Enable Cohesive Option: No
     Sediment Transport Potential: None
     Fall Velocity Method: Rubey

     Enable Quality Routing: No
End:

Source: Inflow
     Last Modified Date: 28 June 2022
     Last Modified Time: 20:36:57
     Canvas X: 123.72304199772998
     Canvas Y: 1461.9750283768444
     From Canvas X: 123.72304199772998
     From Canvas Y: 1461.9750283768444
     Downstream: Tuttle_Creek

     Flow Method: GAGE_FLOW
     Flow Gage: Water_Inflow
     End Flow Method:

     Sediment Method: GAGE_SEDIMENT
     Sediment Gage: Sediment_inflow
     Gradation Curve Name: Inflow_gradation
     End Sediment Method:
End:

Reservoir: Tuttle_Creek
     Last Modified Date: 28 June 2022
     Last Modified Time: 21:08:05
     Canvas X: 1485.8115777525527
     Canvas Y: 139.61407491486898
     From Canvas X: 1485.8115777525527
     From Canvas Y: 139.61407491486898
     Downstream: Outflow

     Route: Controlled Outflow
     Observed Pool Elevation Gage: Lake_elevation
     Routing Curve: Elevation-Area
     Initial Elevation: 1030
     Elevation-Area Table: 1957_Survey
     Adaptive Control: On
     Main Tailwater Condition: None
     Auxiliary Tailwater Condition: None

     Release: Gage Release
     Release Outlet: Main
     Release Gage Name: Water_outflow
     End Release:

     Evaporation Method: Zero Evaporation
     End Evaporation:

     Sediment Method: Brune Variable-Trap
     Update Reservoir Capacity: Yes
     Deposition Shape: Elongated Taper
     Use Water Temperature Gage: No
     Average Water Temperature: 55.0
     Elevation At Capacity: 1075
     Annual Inflow Volume: 1560000
     Constant A: 100
     Constant B: 7.71
     Use Percent Annual Inflow Gage: No
     End Sediment Method: 
End:

Sink: Outflow
     Last Modified Date: 10 May 2022
     Last Modified Time: 20:18:44
     Canvas X: 2660.218022765155
     Canvas Y: -948.8515031927218
     From Canvas X: 2660.218022765155
     From Canvas Y: -948.8515031927218
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
End:

Basin Spatial Properties:
End:

Basin Schematic Properties:
     Last View N: 1461.9750283768444
     Last View S: -948.8515031927218
     Last View W: 123.72304199772998
     Last View E: 2660.218022765155
     Maximum View N: 1461.9750283768444
     Maximum View S: -948.8515031927218
     Maximum View W: 123.72304199772998
     Maximum View E: 2660.218022765155
     Extent Method: Manual
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
