Basin: Brand_Canyon_USGS_LT
     Last Modified Date: 24 January 2022
     Last Modified Time: 16:06:57
     Version: 4.10
     Filepath Separator: \
     Unit System: Metric
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: Yes
     Sediment Grade Scale: SIMPLE_4
     Sediment Properties: 
     Sediment Specific Gravity: 2.65
     Unit Weight Sand Gravel: 2200
     Unit Weight Silt: 1800
     Unit Weight Clay: 1600
     End Sediment Properties: 
     Enable Cohesive Option: No
     Sediment Transport Potential: None
     Fall Velocity Method: Rubey

     Enable Quality Routing: No
End:

Subbasin: Brand_Canyon
     Last Modified Date: 2 February 2022
     Last Modified Time: 18:16:19
     Latitude Degrees:  34.19305555555555
     Longitude Degrees: -118.26638888888888
     Canvas X: -6620911.9445661
     Canvas Y: 4836154.66214424
     Area: 2.6263
     Downstream: Brand_DB

     Discretization: None
     File: Brand_Canyon_USGS_LT.sqlite

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: Initial+Constant
     Percent Impervious Area: 0.0
     Initial Loss: 2
     Constant Loss Rate: 1

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.7
     Storage Coefficient: 1.7
     Time Area Method: Default

     Baseflow: None

     Erosion: None
End:

Reservoir: Brand_DB
     Last Modified Date: 2 February 2022
     Last Modified Time: 18:16:25
     Canvas X: -6624140.95647279
     Canvas Y: 4834311.0256401105
     From Canvas X: -6624398.549894146
     From Canvas Y: 4834490.741980587

     Route: Controlled Outflow
     Routing Curve: Elevation-Storage-Area
     Initial Elevation: 262
     Elevation-Storage Table: Brand_DB
     Elevation-Area Table: Brand_DB
     Adaptive Control: On
     Main Tailwater Condition: None
     Auxiliary Tailwater Condition: None

     Spillway: Broad-Crested Spillway
     Spillway Outlet: Main
     Spillway Crest Length: 18.288
     Spillway Crest Elevation: 271.272
     Spillway Coefficient: 1.66
     End Spillway:

     Evaporation Method: Zero Evaporation
     End Evaporation:

     Sediment Method: Pass-Through
     Update Reservoir Capacity: No
     Deposition Shape: None
     End Sediment Method: 
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     2D Connection Layer:
          Layer shown: No
     End Layer:
     Element Layer:
          Name: Subbasins
          Layer shown: Yes
     End Layer:
     Discretization Layer:
          Layer shown: Yes
     End Layer:
     Breakpoint Layer:
          Layer shown: No
     End Layer:
     Base Layer:
          Name: Identified Streams
          Layer shown: No
          Properties Filename: maps\streams5706080242022.xml
     End Layer:
     Base Layer:
          Name: Flow Accumulation
          Layer shown: No
          Properties Filename: maps\flowaccum5706080242022.xml
     End Layer:
     Base Layer:
          Name: Flow Direction
          Layer shown: No
          Properties Filename: maps\flowdir5706080242022.xml
     End Layer:
     Base Layer:
          Name: Sink Locations
          Layer shown: No
          Properties Filename: maps\sinklocs5706080242022.xml
     End Layer:
     Base Layer:
          Name: Sink Fill
          Layer shown: No
          Properties Filename: maps\sinkfill5706080242022.xml
     End Layer:
     Base Layer:
          Name: Terrain
          Layer shown: Yes
          Properties Filename: maps\elevation5706080242022.xml
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["MMC_Standard",GEOGCS["NAD83",DATUM["North_American_Datum_1983",SPHEROID["GRS 1980",6378137,298.257222101004,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","6269"]],PRIMEM["Greenwich",0],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4269"]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["latitude_of_center",23],PARAMETER["longitude_of_center",-96],PARAMETER["standard_parallel_1",29.5],PARAMETER["standard_parallel_2",45.5],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["US survey foot",0.304800609601219,AUTHORITY["EPSG","9003"]],AXIS["Easting",EAST],AXIS["Northing",NORTH]]
     Terrain: NED_10m_Brand_DB
     Threshold: 2.0
     Break Point: Brand DB
          X Coordinate: -6624127.2076057615
          Y Coordinate: 4834326.642112749
     End Break Point:
     reach_prefix: R_
     junction_insert: true
     junction_prefix: J_
     subbasin_prefix: S_
End:

Basin Schematic Properties:
     Last View N: 4836154.66214424
     Last View S: 4834329.3054891005
     Last View W: -6624130.349228449
     Last View E: -6620911.9445661
     Maximum View N: 4836154.66214424
     Maximum View S: 4834329.3054891005
     Maximum View W: -6624130.349228449
     Maximum View E: -6620911.9445661
     Extent Method: Elements
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Gray Scale
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
