<?xml version="1.0" encoding="UTF-8"?>
<RunResults>
  <RunName>Test Run</RunName>
  <Description>Basin: Test , Meteorology: SCS 5 in , Control: 48 hr window</Description>
  <ExecutionTime>16Jun2022, 14:21:58</ExecutionTime>
  <StartTime>31Jul2022, 24:00</StartTime>
  <EndTime>02Aug2022, 24:00</EndTime>
  <BasinElement name="Subbasin-1" type="Subbasin">
    <ExecutionTime>16Jun2022, 14:21:58</ExecutionTime>
    <SubbasinArea area="20" units="MI2" />
    <UnitSystem>English</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="20" units="MI2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-CUMULATIVE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-INC//5MIN/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-CUM//5MIN/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Air Temperature" displayString="Air Temperature" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/TEMPERATURE-AIR//5MIN/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Daily Average Temperature" displayString="Daily Average Temperature" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/TEMPERATURE-AVERAGE//1DAY/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Daily Minimum Temperature" displayString="Daily Minimum Temperature" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/TEMPERATURE-MINIMUM//1DAY/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Daily Maximum Temperature" displayString="Daily Maximum Temperature" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/TEMPERATURE-MAXIMUM//1DAY/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Reference ET" displayString="Reference Evapotranspiration" />
        <DssFileName>SCS_5_in.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-REFERENCE//5MIN/MET:SCS 5 in/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/EXCESS-CANOPY//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-POTENTIAL//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-CANOPY//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-CANOPY//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/INFILTRATION//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/PERC-SOIL//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Moisture Deficit" displayString="Moisture Deficit" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/MOISTURE DEFICIT//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/SATURATION FRACTION//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS-CUM//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS-CUM//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-DIRECT//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-BASE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Subbasin-1/AQUIFER RECHARGE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="CFS" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Jul2022, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="CFS" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="31Jul2022, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="AC-FT" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="IN" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="CFS" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="29.0460446" units="CFS" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="01Aug2022, 02:05" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="2385.1277722" units="CFS" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Aug2022, 18:25" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="2387.0422688" units="AC-FT" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="2.2378522" units="IN" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="600.8649226" units="CFS" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="CFS" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="31Jul2022, 24:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="1966.1114337" units="CFS" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="01Aug2022, 18:20" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="1456.7170015" units="AC-FT" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="1.3656722" units="IN" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="366.5777381" units="CFS" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="23.8006600" units="CFS" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="01Aug2022, 11:45" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="431.3905507" units="CFS" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="01Aug2022, 22:55" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="930.3252674" units="AC-FT" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="0.8721800" units="IN" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="234.2871845" units="CFS" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="0.5664707" units="IN" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="01Aug2022, 11:50" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="4.8833682" units="IN" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="5208.9258574" units="AC-FT" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="0.2277847" units="IN" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="01Aug2022, 11:40" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="3.5176904" units="IN" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="3752.2029737" units="AC-FT" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="0.5268874" units="IN" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="01Aug2022, 11:50" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="1.3656778" units="IN" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="1456.7228837" units="AC-FT" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Junction-1" type="Junction">
    <ExecutionTime>16Jun2022, 14:21:58</ExecutionTime>
    <UnitSystem>English</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="20" units="MI2" />
    <ObservedFlowGage name="Junction Observed" />
    <FlowLink upstreamName="Subbasin-1" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-CUMULATIVE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Observed Flow" displayString="Observed Flow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-OBSERVED//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Residual Flow" displayString="Residual Flow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-RESIDUAL//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Observed Flow" displayString="Cumulative Observed Flow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-OBSERVED-CUMULATIVE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Test_Run.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-COMBINE//5MIN/RUN:Test Run/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="29.0460446" units="CFS" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="01Aug2022, 02:05" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="2385.1277722" units="CFS" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="01Aug2022, 18:25" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="2387.0422688" units="AC-FT" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="2.2378522" units="IN" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="600.8649226" units="CFS" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="29.0460446" units="CFS" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="01Aug2022, 02:05" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="2385.1277722" units="CFS" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Aug2022, 18:25" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="2387.0422688" units="AC-FT" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="2.2378522" units="IN" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="600.8649226" units="CFS" />
      <StatisticMeasure type="Observed Flow Minimum" displayString="Minimum Observed Flow" value="29.1794175" units="CFS" />
      <StatisticMeasure type="Observed Flow Minimum Time" displayString="Time of Minimum Observed Flow" value="01Aug2022, 01:40" />
      <StatisticMeasure type="Observed Flow Maximum" displayString="Maximum Observed Flow" value="4305.1027206" units="CFS" />
      <StatisticMeasure type="Observed Flow Maximum Time" displayString="Time of Maximum Observed Flow" value="01Aug2022, 15:45" />
      <StatisticMeasure type="Observed Flow Volume" displayString="Observed Flow Volume" value="3658.6256106" units="AC-FT" />
      <StatisticMeasure type="Observed Flow Depth" displayString="Observed Flow Depth" value="3.4299617" units="IN" />
      <StatisticMeasure type="Observed Flow Average" displayString="Observed Flow Average" value="920.8140911" units="CFS" />
      <StatisticMeasure type="Observed Flow RMSE Stdev" displayString="Observed Flow RMSE Stdev" value="0.5685262" units="CFS" />
      <StatisticMeasure type="Observed Flow Nash Sutcliffe" displayString="Observed Flow Nash Sutcliffe" value="0.6767780" units="" />
      <StatisticMeasure type="Observed Flow Percent Bias" displayString="Observed Flow Percent Bias" value="-34.7463371" units="" />
      <StatisticMeasure type="Observed Flow Coefficient of Determination" displayString="Observed Flow Coefficient of Determination" value="0.8703825" units="" />
    </Statistics>
  </BasinElement>
</RunResults>

