

Performing Simulation for Ensemble--0

Starting compute at Sat Jun 08 20:09:25 MDT 2019

Performing Simulation for Ensemble--0
Running ResSim alternative Ensemble--0

Running ResSim
DssFile=C:/Users/nfriesen/Research Triangle Institute/IWR Reservoir Training - Documents/Training Materials/Workshop7/Solution/rss/EnsemblePeriod/simulation.dss
Using Compute Launcher Default Compute Launcher

Using Alternative's timestep of 1DAY

ResSim Compute

Build Version: 3.3.1.117R, 			   March 2017 

Simulation Time Window:
  Lookback	: 01Jan2101 2400
  Start	: 02Jan2101 2400
  End	: 31Dec2200 2400

  Time Step: 1 DAY
ResSim

Initializing Simulation
ResSim Initializing
==========================================================================================
Memory Size needed for TSData = 146 MB
Max Memory            = 3200.0 MB
Total Memory          = 553.0 MB
Free Memory           = 349.0 MB
Used Memory           = 203.0 MB
Max Available Memory  = 2996.0 MB
Minimum Number of TimeWindowBlocks Needed = 1.0
Size of each block = 36523.0 days
==========================================================================================
Initialization Start

Program-Determined Flow Computation Method: Period Average

  Flow Computation Method: Period Average
Compute Initialization Complete
Initialization Complete


Computing Cumulative Local Flow

ResSim Cumulative Local Flow

Ordering Elements for Compute.
ElementGraph: Block   0,  Num Elem  1
ElementGraph: Block   1,  Num Elem  1
ElementGraph: Block   2,  Num Elem  1
ElementGraph: Order   0, Block   0,  Elem  Upper Inflow
ElementGraph: Order   1, Block   1,  Elem  Upper Res
ElementGraph: Order   2, Block   2,  Elem  Upper Outflow
Loading Input Timeseries
RssRun.checkTSRecords: attempting to get DSSFileManager wrapper
C:/Users/nfriesen/Research Triangle Institute/IWR Reservoir Training - Documents/Training Materials/Workshop7/Solution/rss/EnsemblePeriod/simulation.dss::/PURPLE RIVER/UPPER/FLOW_INC//1DAY/001/ Number Read 36529

Starting Computations.
Computing Hindcast
Computing Forecast

Saving ResSim time-series output
Saving ResSim time-series output

Computing Unregulated Flow

ResSim Unregulated Flow

Ordering Elements for Compute.
ElementGraph: Block   0,  Num Elem  1
ElementGraph: Block   1,  Num Elem  1
ElementGraph: Block   2,  Num Elem  1
ElementGraph: Order   0, Block   0,  Elem  Upper Inflow
ElementGraph: Order   1, Block   1,  Elem  Upper Res
ElementGraph: Order   2, Block   2,  Elem  Upper Outflow
Loading Input Timeseries
C:/Users/nfriesen/Research Triangle Institute/IWR Reservoir Training - Documents/Training Materials/Workshop7/Solution/rss/EnsemblePeriod/simulation.dss::/PURPLE RIVER/UPPER/FLOW_INC//1DAY/001/ Number Read 36529

Starting Computations.
Computing Hindcast
Computing Forecast

Saving ResSim time-series output
Saving ResSim time-series output
Yield Analysis Compute 1


Computing Regulated Flow

ResSim Regulated Flow

Ordering Elements for Compute.
ElementGraph: Block   0,  Num Elem  1
ElementGraph: Block   1,  Num Elem  1
ElementGraph: Block   2,  Num Elem  1
ElementGraph: Order   0, Block   0,  Elem  Upper Inflow
ElementGraph: Order   1, Block   1,  Elem  Upper Res
ElementGraph: Order   2, Block   2,  Elem  Upper Outflow

Iteration Block Order for Compute Type - Regulated Flow
Block	Elem ID	Element Name
0	8	Upper Inflow
1	9	Upper Res
2	7	Upper Outflow


Loading Input Timeseries
C:/Users/nfriesen/Research Triangle Institute/IWR Reservoir Training - Documents/Training Materials/Workshop7/Solution/rss/EnsemblePeriod/simulation.dss::/PURPLE RIVER/UPPER/FLOW_INC//1DAY/001/ Number Read 36529

Starting Computations.
Computing Hindcast
Computing Forecast
Computing Operations for Block 1: 1 Elements, 1 Routing Steps, PASS 1
Computing Operations for Block 1: 1 Elements, 1 Routing Steps, PASS 2
Computing Operations for Block 1: 1 Elements, 1 Routing Steps, PASS 3
Computing Operations for Block 1: 1 Elements, 1 Routing Steps, PASS 4

Saving ResSim time-series output
Saving ResSim time-series output
Yield Analysis Rule: "Min Release"

   Demand Scales:

      Max Limit Factor = 1.000000, Min Limit Factor = 0.000000, Trial Factor = 1.000000

   Average Annual Demand = 1496.098555 cfs

   Critical Period: 07May2102 to 05Dec2106

   Minimum Storage on 09Oct2105 is 867000.000000 ac-ft

   Lower Limit of Conservation Pool = 867000.000000 ac-ft; Storage Tolerance = 1000.000000 ac-ft

   Maximum Demand Shortage = 0.000000 cfs; Flow Tolerance = 10.000000 cfs

   Convergence Test: Maximum Demand Shortage Within Rule Tolerance = PASS

   Convergence Test: Within Storage Range of Limit Storage and Limit Storage plus Tolerance = PASS

 

Yield Analysis Compute 1 converged with Demand Scale = 1496.098555 cfs

 


ResSim Compute Complete

Saving output
ResSim Compute Complete
Total Compute Time 6 Seconds.

ResSim Compute Complete for Ensemble--0

