Basin: FRA
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:14:07
     Version: 4.13
     Filepath Separator: \
     Unit System: English
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No
     Unregulated Output Required: No

     Enable Sediment Routing: No
End:

Subbasin: WF Russian
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.28611111111111
     Longitude Degrees: -123.26333333333334
     Canvas X: -7548621.380490861
     Canvas Y: 7024440.943949957
     Label X: 16.0
     Label Y: 16.0
     Area: 101.29
     Downstream: Ukiah Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.3
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 1.7
     Initial Deficit: 7
     Maximum Deficit: 20
     Percolation Rate: 0.1
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 6
     Storage Coefficient: 3
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Ukiah Gage
     Description: Generic junction
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:15:13
     Canvas X: -7529825.245499488
     Canvas Y: 6982688.337715932
     Label X: -95.0
     Label Y: 13.0
     Computation Point: Yes
     Downstream: Conf
End:

Junction: Conf
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:13:49
     Canvas X: -7531348.094585842
     Canvas Y: 6976820.748226186
     Downstream: Russian 75
End:

Reach: Russian 75
     Last Modified Date: 14 January 2016
     Last Modified Time: 00:01:05
     Canvas X: -7534872.858095293
     Canvas Y: 6948266.698244784
     From Canvas X: -7531348.094585842
     From Canvas Y: 6976820.748226186
     Label X: 16.0
     Label Y: 16.0
     Downstream: Below Ukiah

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: Ukiah
     Channel Loss: None
End:

Subbasin: Russian 70
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.16361111111111
     Longitude Degrees: -123.21305555555556
     Canvas X: -7550293.498079511
     Canvas Y: 6977621.651467753
     Label X: -97.0
     Label Y: -5.0
     Area: 84.265
     Downstream: Below Ukiah

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.35
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 3.8
     Initial Deficit: 12
     Maximum Deficit: 20
     Percolation Rate: 0.05
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 7
     Storage Coefficient: 8
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Below Ukiah
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:01:50
     Canvas X: -7534872.858095293
     Canvas Y: 6948266.698244784
     Label X: 18.0
     Label Y: 16.0
     Downstream: Russian 65
End:

Reach: Russian 65
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:01:56
     Canvas X: -7530971.250388443
     Canvas Y: 6915930.75649646
     From Canvas X: -7534872.858095293
     From Canvas Y: 6948266.698244784
     Downstream: Hopland Gage

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: Hopland
     Channel Loss: None
End:

Subbasin: Russian 60
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.06916666666667
     Longitude Degrees: -123.17722222222223
     Canvas X: -7550107.707236327
     Canvas Y: 6940269.356953479
     Label X: -79.0
     Label Y: 19.0
     Area: 72.197
     Downstream: Hopland Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.35
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.3
     Initial Deficit: 12
     Maximum Deficit: 20
     Percolation Rate: 0.05
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 8
     Storage Coefficient: 9
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Hopland Gage
     Description: UserPoint6
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:14:51
     Canvas X: -7530971.250388443
     Canvas Y: 6915930.75649646
     Label X: 16.0
     Label Y: 16.0
     Computation Point: Yes
     Downstream: Russian 55
End:

Reach: Russian 55
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:02:27
     Canvas X: -7524654.361720209
     Canvas Y: 6857004.612776377
     From Canvas X: -7530971.250388443
     From Canvas Y: 6915930.75649646
     Label X: 16.0
     Label Y: 16.0
     Downstream: Cloverdale Gage

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: Cloverdale
     Channel Loss: None
End:

Subbasin: Russian 50
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.94944444444444
     Longitude Degrees: -123.09305555555555
     Canvas X: -7550622.377478898
     Canvas Y: 6896330.714712584
     Label X: -64.0
     Label Y: 23.0
     Area: 139.55
     Downstream: Cloverdale Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.2
     Initial Deficit: 8
     Maximum Deficit: 20
     Percolation Rate: 0.125
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 7.5
     Storage Coefficient: 7.5
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Cloverdale Gage
     Description: UserPoint7
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:14:48
     Canvas X: -7524654.361720209
     Canvas Y: 6857004.612776377
     Label X: -9.0
     Label Y: 20.0
     Computation Point: Yes
     Downstream: Russian 45b
End:

Reach: Russian 45b
     Last Modified Date: 23 November 2015
     Last Modified Time: 22:36:45
     Canvas X: -7518489.9679386625
     Canvas Y: 6833418.839191702
     From Canvas X: -7524654.361720209
     From Canvas Y: 6857004.612776377
     Label X: 16.0
     Label Y: 16.0
     Downstream: Big Sulfur Trib

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Big Sulfur Cr
     Channel Loss: None
End:

Subbasin: Big Sulphur Cr
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.800187
     Longitude Degrees: -122.854155
     Canvas X: -7464033.989665211
     Canvas Y: 6811433.506348384
     Label X: 16.0
     Label Y: 16.0
     Area: 84.898
     Downstream: Big Sulfur Trib

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.4
     Initial Deficit: 10
     Maximum Deficit: 20
     Percolation Rate: 0.30
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 5.2
     Storage Coefficient: 5.2
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Big Sulfur Trib
     Description: Generic junction
     Last Modified Date: 5 May 2016
     Last Modified Time: 23:58:15
     Canvas X: -7518489.9679386625
     Canvas Y: 6833418.839191702
     Label X: 16.0
     Label Y: 16.0
     Downstream: Russian 45
End:

Reach: Russian 45
     Last Modified Date: 23 November 2015
     Last Modified Time: 22:37:00
     Canvas X: -7498195.81454483
     Canvas Y: 6787756.9940555785
     From Canvas X: -7518489.9679386625
     From Canvas Y: 6833418.839191702
     Label X: 16.0
     Label Y: 16.0
     Downstream: Geyserville

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Geyserville
     Channel Loss: None
End:

Subbasin: Russian 40
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.793908
     Longitude Degrees: -122.992182
     Canvas X: -7529313.516415373
     Canvas Y: 6815830.572917047
     Label X: -62.0
     Label Y: 22.0
     Area: 68.121
     Downstream: Geyserville

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 2.2
     Initial Deficit: 10
     Maximum Deficit: 20
     Percolation Rate: 0.30
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 4.1
     Storage Coefficient: 4.1
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Geyserville
     Description: UserPoint9
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:02:57
     Canvas X: -7498195.81454483
     Canvas Y: 6787756.9940555785
     Label X: 16.0
     Label Y: 16.0
     Downstream: Russian 35
End:

Reach: Russian 35
     Last Modified Date: 23 November 2015
     Last Modified Time: 22:37:13
     Canvas X: -7490416.389077193
     Canvas Y: 6747168.687267913
     From Canvas X: -7498195.81454483
     From Canvas Y: 6787756.9940555785
     Label X: 16.0
     Label Y: 16.0
     Downstream: Healdsburg Gage

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Healdsburg
     Channel Loss: None
End:

Subbasin: Russian 30
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.65833333333333
     Longitude Degrees: -122.75638888888889
     Canvas X: -7459975.158986445
     Canvas Y: 6761712.830533493
     Label X: 10.0
     Label Y: 0.0
     Area: 135.47
     Downstream: Healdsburg Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.6
     Initial Deficit: 10
     Maximum Deficit: 20
     Percolation Rate: 0.30
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 4.0
     Storage Coefficient: 4.0
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Healdsburg Gage
     Description: UserPoint10
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:14:43
     Canvas X: -7490416.389077193
     Canvas Y: 6747168.687267913
     Label X: 9.0
     Label Y: 7.0
     Computation Point: Yes
     Downstream: Russian 25d
End:

Reach: Russian 25d
     Last Modified Date: 24 November 2015
     Last Modified Time: 01:11:58
     Canvas X: -7501578.173443802
     Canvas Y: 6740176.05937471
     From Canvas X: -7490416.389077193
     From Canvas Y: 6747168.687267913
     Label X: 5.0
     Label Y: -1.0
     Downstream: J Dry Cr w Russian

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Dry Creek
     Channel Loss: None
End:

Reach: Dry Cr 15
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:14:07
     Canvas X: -7501578.173443802
     Canvas Y: 6740176.05937471
     From Canvas X: -7517465.412182889
     From Canvas Y: 6783322.656836019
     Label X: 1.0
     Label Y: 16.0
     Downstream: J Dry Cr w Russian

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: Dry Cr 15
     Channel Loss: None
End:

Subbasin: Dry Creek 10
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.643028
     Longitude Degrees: -122.96361111111112
     Canvas X: -7537431.177772907
     Canvas Y: 6765205.515227104
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -46.0
     Label Y: 28.0
     Area: 84.120
     Downstream: J Dry Cr w Russian

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.6
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 8.8
     Storage Coefficient: 19.25
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J Dry Cr w Russian
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:04:50
     Canvas X: -7501578.173443802
     Canvas Y: 6740176.05937471
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -3.0
     Label Y: 2.0
     Downstream: Russian 25c
End:

Reach: Russian 25c
     Last Modified Date: 24 November 2015
     Last Modified Time: 01:11:58
     Canvas X: -7517813.496158868
     Canvas Y: 6709734.82928396
     From Canvas X: -7501578.173443802
     From Canvas Y: 6740176.05937471
     Label X: 16.0
     Label Y: 16.0
     Downstream: J Conf SantaRosa w Russian

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Santa Rosa Cr
     Channel Loss: None
End:

Subbasin: Laguna
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.3689
     Longitude Degrees: -122.733373
     Canvas X: -7490078.153187296
     Canvas Y: 6644793.538423696
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 16.0
     Label Y: 16.0
     Area: 79.972
     Downstream: J  Laguna

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 15
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 8.5
     Storage Coefficient: 9.35
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J  Laguna
     Description: UserPoint12
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:03:26
     Canvas X: -7511725.250140718
     Canvas Y: 6678617.127413417
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 6.0
     Label Y: -7.0
     Reference Flow: 6700
     Reference Flow Label: 1 Jan 2006
     Downstream: Santa Rosa 15b
End:

Reach: Santa Rosa 15b
     Last Modified Date: 19 April 2019
     Last Modified Time: 22:13:39
     Canvas X: -7509357.598911437
     Canvas Y: 6686058.316991156
     From Canvas X: -7511725.250140718
     From Canvas Y: 6678617.127413417
     Label X: -70.0
     Label Y: -3.0
     Downstream: J Conf SantaRosa / Laguna

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 12000
     Energy Slope: 0.00001
     Mannings n: 0.04
     Left Mannings n: 0.06
     Right Mannings n: 0.06
     Cross Section Name: Santa Rosa Mid
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: Santa Rosa Cr 20
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.45055555555556
     Longitude Degrees: -122.65333333333334
     Canvas X: -7468769.292123772
     Canvas Y: 6679293.599193212
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 16.0
     Label Y: 16.0
     Area: 73.500
     Downstream: Santa Rosa Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 30
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 7.6
     Storage Coefficient: 12.1
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Santa Rosa Gage
     Description: UserPoint11
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:04:29
     Canvas X: -7497857.578654932
     Canvas Y: 6685381.845211362
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -5.0
     Label Y: -1.0
     Reference Flow: 6400
     Reference Flow Label: 1 Jan 2006
     Downstream: Santa Rosa 15
End:

Reach: Santa Rosa 15
     Last Modified Date: 19 April 2019
     Last Modified Time: 22:13:39
     Canvas X: -7509357.598911437
     Canvas Y: 6686058.316991156
     From Canvas X: -7497857.578654932
     From Canvas Y: 6685381.845211362
     Label X: -28.0
     Label Y: 18.0
     Downstream: J Conf SantaRosa / Laguna

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 10000
     Energy Slope: 0.001
     Mannings n: 0.04
     Left Mannings n: 0.06
     Right Mannings n: 0.06
     Cross Section Name: Santa Rosa Mid
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: J Conf SantaRosa / Laguna
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:04:42
     Canvas X: -7509357.598911437
     Canvas Y: 6686058.316991156
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -145.0
     Label Y: -1.0
     Downstream: Santa Rosa 10
End:

Reach: Santa Rosa 10
     Last Modified Date: 19 April 2019
     Last Modified Time: 22:13:39
     Canvas X: -7517813.496158868
     Canvas Y: 6709734.82928396
     From Canvas X: -7509357.598911437
     From Canvas Y: 6686058.316991156
     Label X: -38.0
     Label Y: -2.0
     Downstream: J Conf SantaRosa w Russian

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 37000
     Energy Slope: 0.0012
     Mannings n: 0.035
     Left Mannings n: 0.06
     Right Mannings n: 0.05
     Cross Section Name: Santa Rosa Lower
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: Santa Rosa Cr 10
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.514141
     Longitude Degrees: -122.744146
     Canvas X: -7473842.83047223
     Canvas Y: 6707367.17805468
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 16.0
     Label Y: 16.0
     Area: 99.321
     Downstream: J Conf SantaRosa w Russian

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 5.2
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 8.4
     Storage Coefficient: 18.7
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J Conf SantaRosa w Russian
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:04:45
     Canvas X: -7517813.496158868
     Canvas Y: 6709734.82928396
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 16.0
     Label Y: 16.0
     Downstream: Russian 25b
End:

Reach: Russian 25b
     Last Modified Date: 24 November 2015
     Last Modified Time: 01:11:58
     Canvas X: -7527622.336965887
     Canvas Y: 6710073.065173858
     From Canvas X: -7517813.496158868
     From Canvas Y: 6709734.82928396
     Label X: -60.0
     Label Y: -14.0
     Downstream: J Conf Green w Russian

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Green Valley
     Channel Loss: None
End:

Subbasin: Green Valley
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.423681
     Longitude Degrees: -122.887982
     Canvas X: -7526607.629296196
     Canvas Y: 6684705.373431567
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 0.0
     Label Y: -20.0
     Area: 37.872
     Downstream: J Conf Green w Russian

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 5.1
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 9.6
     Storage Coefficient: 20.9
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J Conf Green w Russian
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:04:46
     Canvas X: -7527622.336965887
     Canvas Y: 6710073.065173858
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -125.0
     Label Y: -6.0
     Downstream: Russian 25a
End:

Reach: Russian 25a
     Last Modified Date: 24 November 2015
     Last Modified Time: 01:11:58
     Canvas X: -7529115.880963907
     Canvas Y: 6717086.667829469
     From Canvas X: -7527622.336965887
     From Canvas Y: 6710073.065173858
     Label X: 27.0
     Label Y: 5.0
     Downstream: Guerneville Gage

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 5
     Storage Outflow Table Name: Guerneville
     Channel Loss: None
End:

Subbasin: Russian 20
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.558064
     Longitude Degrees: -122.878854
     Canvas X: -7526269.393406298
     Canvas Y: 6730367.218567691
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -39.0
     Label Y: 13.0
     Area: 38.899
     Downstream: Guerneville Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 5.0
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 7.0
     Storage Coefficient: 15.4
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Guerneville Gage
     Description: UserPoint13
     Last Modified Date: 7 June 2016
     Last Modified Time: 22:27:14
     Canvas X: -7529115.880963907
     Canvas Y: 6717086.667829469
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -9.0
     Label Y: 30.0
     Computation Point: Yes
     Downstream: Russian 15b
End:

Reach: Russian 15b
     Last Modified Date: 12 February 2016
     Last Modified Time: 23:45:10
     Canvas X: -7567361.726471701
     Canvas Y: 6711389.772930543
     From Canvas X: -7529115.880963907
     From Canvas Y: 6717086.667829469
     Label X: -18.0
     Label Y: -10.0
     Downstream: J Conf Austin w Russian

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 2
     Storage Outflow Table Name: Austin
     Channel Loss: None
End:

Subbasin: Austin Cr
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.574218
     Longitude Degrees: -123.089648
     Canvas X: -7569225.351423244
     Canvas Y: 6748631.9566221405
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -21.0
     Label Y: 21.0
     Area: 62.388
     Downstream: J Austin Cr

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.3
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 6.7
     Storage Coefficient: 6.7
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J Austin Cr
     Description: Generic junction
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:03:48
     Canvas X: -7567534.171973758
     Canvas Y: 6726646.623778821
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -88.0
     Label Y: 4.0
     Reference Flow: 0
     Reference Flow Label: N/A for 86 Event
     Downstream: Austin Cr 10
End:

Reach: Austin Cr 10
     Last Modified Date: 19 April 2019
     Last Modified Time: 22:13:39
     Canvas X: -7567361.726471701
     Canvas Y: 6711389.772930543
     From Canvas X: -7567534.171973758
     From Canvas Y: 6726646.623778821
     Label X: -15.0
     Label Y: 7.0
     Downstream: J Conf Austin w Russian

     Route: Muskingum Cunge
     Channel: 8-point
     Length: 21000
     Energy Slope: 0.0031
     Mannings n: 0.04
     Left Mannings n: 0.06
     Right Mannings n: 0.06
     Cross Section Name: Austin Cr
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Junction: J Conf Austin w Russian
     Description: Generic junction
     Last Modified Date: 30 November 2015
     Last Modified Time: 19:41:17
     Canvas X: -7567361.726471701
     Canvas Y: 6711389.772930543
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -29.0
     Label Y: -37.0
     Downstream: Russian 15a
End:

Reach: Russian 15a
     Last Modified Date: 30 November 2015
     Last Modified Time: 19:45:22
     Canvas X: -7588763.221514255
     Canvas Y: 6710461.611470646
     From Canvas X: -7567361.726471701
     From Canvas Y: 6711389.772930543
     Label X: -46.0
     Label Y: 11.0
     Downstream: Ocean Outlet

     Route: Modified Puls
     Initial Variable: Combined Inflow
     Number of Reaches: 1
     Storage Outflow Table Name: Outlet
     Channel Loss: None
End:

Subbasin: Russian 10
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.478177
     Longitude Degrees: -123.016854
     Canvas X: -7562798.869515197
     Canvas Y: 6697558.33724766
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -42.0
     Label Y: -29.0
     Area: 83.908
     Downstream: Ocean Outlet

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 2.7
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 3.2
     Storage Coefficient: 3.2
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Ocean Outlet
     Description: Outlet2
     Last Modified Date: 30 November 2015
     Last Modified Time: 19:45:22
     Canvas X: -7588763.221514255
     Canvas Y: 6710461.611470646
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -72.0
     Label Y: -4.0
End:

Subbasin: Dry Creek 30
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.82555555555556
     Longitude Degrees: -123.15333333333334
     Canvas X: -7559211.458552312
     Canvas Y: 6858119.357835477
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: 16.0
     Label Y: 16.0
     Area: 87.438
     Downstream: J Dry Cr

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.1
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 10.8
     Storage Coefficient: 10.8
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: J Dry Cr
     Description: UserPoint8
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:02:18
     Canvas X: -7549364.5438635945
     Canvas Y: 6813715.346314657
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -70.0
     Label Y: -5.0
     Downstream: Dry Cr25
End:

Reach: Dry Cr25
     Description: Short routing reach into reservoir
     Last Modified Date: 19 April 2019
     Last Modified Time: 22:13:39
     Canvas X: -7528741.760270243
     Canvas Y: 6798108.915487255
     From Canvas X: -7549364.5438635945
     From Canvas Y: 6813715.346314657
     Label X: -60.0
     Label Y: -8.0
     Downstream: Warm Springs Dam Inflow

     Route: Muskingum Cunge
     Channel: Trapezoid
     Length: 2000
     Energy Slope: 0.001
     Mannings n: 0.035
     Bottom Width: 250
     Side Slope: 4
     Initial Variable: Combined Inflow
     Space-Time Method: Automatic DX and DT
     Index Parameter Type: Index Celerity
     Index Celerity: 5
     Maximum Depth Iterations: 20
     Maximum Route Step Iterations: 30
     Channel Loss: None
End:

Subbasin: Dry Creek 20
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  38.704936
     Longitude Degrees: -123.084061
     Canvas X: -7558468.2951795785
     Canvas Y: 6796065.216212238
     From Canvas X: -202635.3680990711
     From Canvas Y: -75460.80416265759
     Label X: -102.0
     Label Y: 10.0
     Area: 42.214
     Downstream: Warm Springs Dam Inflow

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.4
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 0.1
     Initial Deficit: 6
     Maximum Deficit: 20
     Percolation Rate: 0.4
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 2.4
     Storage Coefficient: 2.4
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 200
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: Warm Springs Dam Inflow
     Last Modified Date: 26 October 2015
     Last Modified Time: 23:02:20
     Canvas X: -7528741.760270243
     Canvas Y: 6798108.915487255
End:

Subbasin: EF Russian 20
     Last Modified Date: 7 June 2016
     Last Modified Time: 22:31:10
     Latitude Degrees:  39.28611111111111
     Longitude Degrees: -123.095
     Canvas X: -7487218.461079404
     Canvas Y: 7018987.612004277
     Label X: 16.0
     Label Y: 16.0
     Area: 91.875
     Downstream: Capella Gage

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Default Tension-Factor
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.7
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.1
     Surface Albedo: 0.20
     End Surface:

     LossRate: Soil Moisture Account
     Percent Impervious Area: 1.0
     Initial Soil Storage Percent: 70
     Initial Gw1 Storage Percent: 5
     Initial Gw2 Storage Percent: 10
     Soil Maximum Infiltration: 0.3
     Soil Storage Capacity: 10
     Soil Tension Capacity: 7
     Soil Maximum Percolation: 0.1
     Groundwater 1 Storage Capacity: 4
     Groundwater 1 Routing Coefficient: 24
     Groundwater 1 Maximum Percolation: 0.1
     Groundwater 2 Storage Capacity: 10
     Groundwater 2 Routing Coefficient: 150
     Groundwater 2 Maximum Percolation: 0.001

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 5.5
     Storage Coefficient: 4.5
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 0.5
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 24
     GW-2 Initial Flow/Area Ratio: 0
End:

Junction: Capella Gage
     Description: UserPoint4
     Last Modified Date: 9 May 2016
     Last Modified Time: 18:15:00
     Canvas X: -7508490.558363257
     Canvas Y: 6992113.337236054
     Label X: 16.0
     Label Y: 16.0
     Computation Point: Yes
     Downstream: CVD Inflow
End:

Subbasin: EF Russian 10
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.21888888888889
     Longitude Degrees: -123.14972222222222
     Canvas X: -7511033.967853997
     Canvas Y: 6979594.012797339
     Label X: 16.0
     Label Y: 16.0
     Area: 11.823
     Downstream: CVD Inflow

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: Simple
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: Simple
     Initial Canopy Storage Percent: 0.0
     Canopy Storage Capacity: 0.1
     Crop Coefficient: 0.3
     End Canopy:

     Surface: Simple
     Initial Surface Storage Percent: 0.0
     Surface Storage Capacity: 0.25
     Surface Albedo: 0.20
     End Surface:

     LossRate: Deficit Constant
     Percent Impervious Area: 21.7
     Initial Deficit: 7
     Maximum Deficit: 20
     Percolation Rate: 0.075
     Recovery Factor: 1.0

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.2
     Storage Coefficient: 1.2
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Junction: CVD Inflow
     Last Modified Date: 17 May 2017
     Last Modified Time: 17:03:56
     Canvas X: -7519359.60481439
     Canvas Y: 6991762.523221771
End:

Subbasin: EF Russian 20 no losses
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.28611111111111
     Longitude Degrees: -123.095
     Canvas X: -7482457.553422487
     Canvas Y: 7006928.664398901
     From Canvas X: 4279.1492790058255
     From Canvas Y: -16635.35826966539
     Label X: 16.0
     Label Y: 16.0
     Area: 91.875

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 5.5
     Storage Coefficient: 4.5
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 0.5
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 24
     GW-2 Initial Flow/Area Ratio: 0
End:

Subbasin: EF Russian 10 no losses
     Last Modified Date: 22 November 2022
     Last Modified Time: 17:25:19
     Latitude Degrees:  39.21888888888889
     Longitude Degrees: -123.14972222222222
     Canvas X: -7495624.249588276
     Canvas Y: 6976158.667924505
     From Canvas X: 10829.783618426882
     From Canvas Y: -5336.415116325952
     Label X: 16.0
     Label Y: 16.0
     Area: 11.823

     Discretization: File-Specified
     File: regions\RussianRiver.mod

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: None

     Transform: Clark
     Clark Method: Specified
     Time of Concentration: 1.2
     Storage Coefficient: 1.2
     Time Area Method: Default

     Baseflow: Linear Reservoir
     Groundwater Layer: 1
     GW-1 Baseflow Fraction: 0.50
     GW-1 Number Reservoirs: 1
     GW-1 Routing Coefficient: 24
     GW-1 Initial Flow/Area Ratio: 0
     Groundwater Layer: 2
     GW-2 Baseflow Fraction: 0.50
     GW-2 Number Reservoirs: 1
     GW-2 Routing Coefficient: 400
     GW-2 Initial Flow/Area Ratio: 5
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
     Map Layer:
          Filename: maps\basin.shp
          Layer:0
          Display name: basin.shp
          Minimum Scale: Undefined
          Maximum Scale: 2147483647
          Layer shown: Yes
          Properties Filename: maps\basin2834093262022.gdr
     End Layer:
     Map Layer:
          Filename: maps\RR_StreamAligment.shp
          Layer:0
          Display name: RR_StreamAligment.shp
          Minimum Scale: Undefined
          Maximum Scale: 2147483647
          Layer shown: Yes
          Properties Filename: maps\RR_StreamAligment2634093262022.gdr
     End Layer:
End:

Basin Spatial Properties:
     Coordinate System: PROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["NAD83",DATUM["North_American_Datum_1983",SPHEROID["GRS 1980",6378137,298.257222101,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","6269"]],PRIMEM["Greenwich",0],UNIT["Degree",0.0174532925199433]],PROJECTION["Albers_Conic_Equal_Area"],PARAMETER["false_easting",0],PARAMETER["false_northing",0],PARAMETER["longitude_of_center",-96],PARAMETER["standard_parallel_1",29.5],PARAMETER["standard_parallel_2",45.5],PARAMETER["latitude_of_center",23],UNIT["US survey foot",0.304800609601219,AUTHORITY["EPSG","9003"]],AXIS["Easting",EAST],AXIS["Northing",NORTH]]
End:

Basin Schematic Properties:
     Last View N: 7012447.069438802
     Last View S: 6966951.024395252
     Last View W: -7538012.420515981
     Last View E: -7480864.94930274
     Maximum View N: 7051839.9864887055
     Maximum View S: 6625175.856751018
     Maximum View W: -7593153.875868622
     Maximum View E: -7424059.004497287
     Extent Method: Elements Maps
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: Yes
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Default
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
     Map: hec.map.aishape.AiShapeMap
     Map File Name: maps\basin.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: maps\RR_StreamAligment.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\WAT Studies\FINAL Russian River WAT STUDY\RRFIRO160819\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\WAT Studies\FINAL Russian River WAT STUDY\New folder\RRFIRO160825\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\WAT Studies\FINAL Russian River WAT STUDY\RRFIRO160825\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RRFIRO160825\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RRFIRO160909\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RRFIRO160926\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RRFIRO160825_160927\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RRFIRO160825_160927_WO runs\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
     Map: hec.map.aishape.AiShapeMap
     Map File Name: C:\Temp\RR_FIRO_Final\maps\RussianSubbasinsSimple.shp
     Minimum Scale: -2147483648
     Maximum Scale: 2147483647
     Map Shown: Yes
End:

Computation Point: Ukiah Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Hopland Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Cloverdale Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Healdsburg Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Guerneville Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 

Computation Point: Capella Gage
     Parameter Set: 1
     End Parameter Set:
     Parameter Set: 2
     End Parameter Set:
     Parameter Set: 3
     End Parameter Set:
     Parameter Set: 4
     End Parameter Set:
     Parameter Set: 5
     End Parameter Set:

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

     Graph Definition: 
     End Graph Definition: 

End Computation Point: 
