
Results text file opened in Study.
File: Fda_Results.txt opened on Mon Sep 28 13:04:59 2020
	(T:\Data\FDA\v143\_Example Data\_Ending Files\BearCreek_Mix\Fda_Results.txt)
------------------------------------------------------------------------------------------------------------------------
Report Expected Annual Damage by Plans and Analysis Years.
Study:	BearCreek_Mix
Monetary Units:	$1,000's
Version 1.4.3, November 1, 2020;  Less Simple Method  (0.010)                                                                                                                       
Plan	Plan Description	2021	
 Without	Without project condition	    595.89	
 01FW	Floodwall	    194.78	
 02FW+GEO	Floodwall and geotech	    235.86	
 03FW+IE	Floodwall and Interior / Exterior	     88.73	
 04FW+GEO+IE	Floodwall and Geotechnical and Interior/Exterior	    128.62	
 05TransQ_G	Transform flow, Base yr graphical	    546.26	
 06TransQ_A	Transform flow, Base yr analytical	    523.26	
 07FW+GEOA	Floodwall and Geotechnical with added points	    235.86	
 08FW+GEOA+IE	Floodwall, Geotechnical with added points and Interior/Exterior	    128.62	
 09FW+GEOA+IE_A	Analytical Freq; Floodwall, geotech w added pts, int/ext	    131.06	
 10WspStage	Without plan but with stage profiles	    623.76	
 11FW+SQ TRIANG	Floodwall with triangular error distribution on rating curve	    215.16	
 12As	Analytical using synthetic ordinates	    553.88	
 13Am	Log Pearson III Analytic from Moments	    547.56	
 14GQ_UduLog	Graphical Flow-Prob Func, User Def LogNormUncertainty	    600.28	
 15GS_UduNorm	Graphical Stage-Prob Func, User Def Normal Uncertainty	    622.90	
 16GQ_UduTri	Graphical Flow-Prob Func, User Def Triangular Uncertainty	    588.12	
 17GS_UduTri	Graphical Stage-Prob Func, User Def Triangular Uncertainty	    594.45	
 18AmFw	Log Pearson III Analytic from Moments with Floodwall	    196.52	
 19AmFwGeo	Log Pearson III Analytic from Moments, Floodwall w GeoTech	    237.26	
 20GQ_NoUncert	Graphical curve, no uncertainty, same as Without	    564.42	
 21GQ_FwWave	Graphical curve, Floodwall, Wave Overtopping	      4.38	
 22GQ+FW+Wave+Geo	Graphical curve, Floodwall, Wave with Geotechnical	    235.89	
 23GQ_SQnormOrd	Without graphical, rating is normal by ordinate	    595.89	
 24GQ_SQtriOrd	Without graphical, rating is triangle by ordinate	    621.35	
 25GQ_SQtriGlob	Without graphical, rating is triangle Using Global	    621.33	



